{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":9,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-M"]
[]
[]
[]
[]
["","","","","","2MXM40M2V1B","2MXM40M4V1B","2MXM40M3V1B","2MXM50M2V1B"]
["Ventilatori","Shkalla e qarkullimit të ajrit","Ftohje","Super e ulët","m³/min","30","","","34"]
["","","Ngrohje","Super e ulët","m³/min","32","","","34"]
["","","","Super e ulët","cfm","1059","","","1200"]
["","","Ngrohje","Super e ulët","cfm","1130","","","1200"]
["Dimensionet","Njësia","","Lartësia","mm","550","550","550","550"]
["","","","Gjerësia","mm","765","765","765","765"]
["","","","Thellësia","mm","285","285","285","285"]
["Pesha","Njësia","","","kg","36","36","36","41"]
["Motori i ventilatorit","Shpejtësia","Ftohje","Super e ulët","rpm","760","500","500","890"]
["","","Ngrohje","Super e ulët","rpm","820","320","320","890"]
["Compressor","Lloji","","","","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","-10","-10","-10 (2)","-10"]
["","","","Maks.","°CDB","46","46","46 (2)","46"]
["","Ngrohje","Ambienti","Min.","°CWB","-15","-15","-15","-15"]
["","","","Maks.","°CWB","18","18","18","18"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","","46","46"]
["","","","Nom.","dBA","48","","","46"]
["","Ngrohje","","I lartë","dBA","","48","48"]
["","","","Nom.","dBA","50","","","48"]
["Agjenti ftohës","Lloji","","","","R-32","R-32","R-32","R-32"]
["","Mbushja","","","kg","0.88","0.88","0.88","1.15"]
["","Mbushja","","","tCO2Eq","0.6","0.60","0.59","0.8"]
["","GWP","","","","675","675","675","675"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","20","20","20 (1)","20"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 20m)","0.02 (për gjatësinë e tubave që kalojnë 20m)","0.02 (për gjatësinë e tubave që kalojnë 20m)","0.02 (për gjatësinë e tubave që kalojnë 20m)"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","15","15.0","15.0","15"]
["","","IU - IU","Maks.","m","7.5","7.5","7.5","7.5"]
["","Gjatësia totale e tubacioneve","Sistemi","Aktuale","m","30","30","30","30"]
["Aksesore Standarde","Installation manual","","","","Installation manual","1","1","1"]
["","Drain plug","","","","Drain plug","1","1","1"]
["","Screw bag","","","","Screw bag","1","1","1"]
["Furnizimi me energji","Faza","","","","1~","1~","1~","1~"]
["","Frekuenca","","","Hz","50","50","50","50"]
["","Tensioni","","","V","220-240","220-230-240","220-230-240","220-240"]
["Shënime","","","","","","(1) - Për një dhomë"]
["","","","","","","","(1) - Për një dhomë"]
["","","","","","","","(2) - Shiko skicën e veçantë për diapazonin e funksionimit"]
["Aksesore Standarde","Reducer assembly","","","","","","","1"]