{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":62,"n_cols":8,"rows_kept":62,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXS-E"]
[]
[]
[]
[]
["","","","","","3MXS52E4V1B","3MXS52E4V1B2","3MXS52E3V1B"]
["Niveli i presionit të zhurmës","Ngrohje","","Nom.","dBA","47","47"]
["","Ftohje","","Nom.","dBA","46","46"]
["Aksesore Standarde","Manual instalimi","","","","1","1"]
["","Tapë kullimi","","","","1","1"]
["","Komplet reduktorësh","","","","1","1"]
["","Pllakë për rregullimin e drejtimit të ajrit","","","","1","1"]
["Freoni","Charge","","","TCO2Eq","4.2","4.2"]
["","GWP","","","","2,087.5","2,087.5"]
["","Ngarkesa","","","kg","2.0","2.0"]
["","Type","","","","R-410A","R-410A"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Maks.","°C DB","46","46"]
["","","","Min.","°C DB","-10","-10"]
["","Ngrohje","Ambienti","Maks.","°C WB","18","18"]
["","","","Min.","°C WB","-15","-15"]
["Piping connections","Ndryshimi i nivelit","IU - IU","Maks.","m","7.5","7.5"]
["","","IU - OU","Maks.","m","15","15"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 30 m)","0.02 (për gjatësinë e tubave që kalojnë 30 m)"]
["","Gjatësia totale e tubacioneve","Sistemi","Aktuale","m","50","50"]
["Kompresori","Lloji","","","","Kompresor me lëkundje i izoluar hermetikisht","Kompresor me lëkundje i izoluar hermetikisht"]
["Dimensionet","Njësia","","Gjerësia","mm","936","936"]
["","","","Thellësia","mm","300","300"]
["","","","Lartësia","mm","735","735"]
["Pesha","Njësia","","","kg","49","49"]
["Power supply","Faza","","","","1~","1~"]
["","Frekuenca","","","Hz","50","50"]
["","Tensioni","","","V","230","230"]
["Shënime","","","","","(1) - Ftohje: temp. e brendshme 27°CDB, 19.0°CWB; temperatura e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7.5m","(1) - Ftohje: temp. e brendshme 27°CDB, 19.0°CWB; temperatura e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7.5m"]
["","","","","","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7.5m","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7.5m"]
["","","","","","(3) - Përmban gaze të fluorinuara të efektit serrë","(3) - Përmban gaze të fluorinuara të efektit serrë"]
["Dimensionet","Njësia","","Lartësia","mm","","","735"]
["","","","Gjerësia","mm","","","936"]
["","","","Thellësia","mm","","","300"]
["Pesha","Njësia","","","kg","","","49"]
["Kompresori","Lloji","","","","","","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°C DB","","","-10"]
["","","","Maks.","°C DB","","","46"]
["","Ngrohje","Ambienti","Min.","°C WB","","","-15"]
["","","","Maks.","°C WB","","","15.5"]
["Niveli i presionit të zhurmës","Ftohje","","Nom.","dBA","","","46"]
["","Ngrohje","","Nom.","dBA","","","47"]
["Agjenti ftohës","Lloji","","","","","","R-410A"]
["","Mbushja","","","kg","","","2.0"]
["","Mbushja","","","tCO2Eq","","","4.2"]
["","GWP","","","","","","2087.5"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","","","25"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","","","0.02 (për gjatësinë e tubave që kalojnë 30 m)"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","","","15"]
["","","IU - IU","Maks.","m","","","7.5"]
["","Gjatësia totale e tubacioneve","Sistemi","Aktuale","m","","","50"]
["Aksesore Standarde","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["","Air direction adjustment plate","","","","","","1"]
["Furnizimi me energji","Faza","","","","","","1~"]
["","Frekuenca","","","Hz","","","50"]
["","Tensioni","","","V","","","230"]