{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXM-M"]
[]
[]
[]
[]
["","","","","","5MXM90M2V1B"]
["Ventilatori","Shkalla e qarkullimit të ajrit","Ftohje","Super e ulët","m³/min","24.1"]
["","","Ngrohje","Super e ulët","m³/min","24.1"]
["","","","Super e ulët","cfm","851"]
["","","Ngrohje","Super e ulët","cfm","851"]
["Dimensionet","Njësia","","Lartësia","mm","734"]
["","","","Gjerësia","mm","320"]
["","","","Thellësia","mm","868"]
["Pesha","Njësia","","","kg","68"]
["Kompresori","Lloji","","","","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","-10"]
["","","","Maks.","°CDB","46"]
["","Ngrohje","Ambienti","Min.","°C WB","-15"]
["","","","Maks.","°C WB","18"]
["Niveli i presionit të zhurmës","Ftohje","","Nom.","dBA","52"]
["","Ngrohje","","Nom.","dBA","52"]
["Agjenti ftohës","Lloji","","","","R-32"]
["","Mbushja","","","kg","2.4"]
["","Mbushja","","","tCO2Eq","1.6"]
["","GWP","","","","675"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","25"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 30 m)"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","15"]
["","","IU - IU","Maks.","m","7.5"]
["","Gjatësia totale e tubacioneve","Sistemi","Aktuale","m","75"]
["Aksesore Standarde","Installation manual","","","","1"]
["","Drain cap","","","","9"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Furnizimi me energji","Faza","","","","1~"]
["","Frekuenca","","","Hz","50"]
["","Tensioni","","","V","220-240"]