{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-A / AZQS-BY1"]
[]
[]
[]
[]
["","","","","ADEQ100A7VEB / AZQS100B7Y1B","ADEQ125A7VE1B / AZQS125B7Y1B"]
["Kapaciteti ftohës","Nom.","","kW","9.5","12.1 (3)"]
["Ftohja e hapësirës","SEER","","","4.81"]
["","Konsumi vjetor i energjisë","","kWh/a","692"]
["","Kapaciteti","Pdesign","kW","9.50"]
["","Kategoria e efikasitetit të energjisë","","","B"]
["Ngrohja e hapësirës (klimë mesatare)","Kapaciteti","Pdesign","kW","7.60"]
["","SCOP/A","","","3.81"]
["","Kategoria e efikasitetit të energjisë","","","A"]
["","Konsumi vjetor i energjisë","","kWh/a","2,793"]
["Efikasiteti nominal","Annual energy consumption","","kWh","1,480","2,010"]
["","EER","","","3.21","3.01"]
["","COP","","","3.61","3.45"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A","B"]
["","","Ngrohje","","A","B"]
["Kapaciteti ngrohës","Nom.","","kW","10.8","13.5 (4)"]
["Shënime","","","","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së"]
["","","","","(2) - Efikasiteti nominal: ftohje në ngarkesë nominale 35°/27°, ngrohje në ngarkesë nominale 7°/20°","(2) - Efikasiteti nominal: ftohje në ngarkesë nominale 35°/27°, ngrohje në ngarkesë nominale 7°/20°"]