{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":9,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C"]
[]
[]
[]
[]
["","","","","","AHQ71CV1","AHQ100CV1","AHQ125CV1","AHQ140CV1"]
["Fuqia në hyrje","Ngrohje","","Nom.","kW","0.106","0.149"]
["","Ftohje","","Nom.","kW","0.106","0.149"]
["Ventilatori","Presioni i jashtëm statik","","I lartë","Pa","0","0","0","0"]
["","","","I ulët","Pa","0","0","0","0"]
["Kapaciteti ftohës","Kapaciteti total","","Nom.","kW","","","12.10","13.00"]
["Kapaciteti i ngrohjes","Kapaciteti total","","Nom.","kW","","","13.5","15.5"]
["Veshja e jashtme","Ngjyra","","","","E bardhë","E bardhë","E bardhë","E bardhë"]
["","Materiali","","","","Çelik i galvanizuar","Çelik i galvanizuar"]
["Dimensionet","Njësia","","Lartësia","mm","260","260","260","285"]
["","","","Gjerësia","mm","1320","1538","1790","1900"]
["","","","Thellësia","mm","634","634","634","680"]
["Pesha","Njësia","","","kg","38","45","65","70"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","23.8","31.1","34.4","43.9"]
["","","","Nom.","m³/min","21.3","27.8","31","39"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","","","31","39"]
["","","","I ulët","m³/min","18.9","24.8","27.2","28.3"]
["","","Ngrohje","I lartë","m³/min","23.8","31.1","34.4","43.9"]
["","","","Nom.","m³/min","21.3","27.8","30.6","39.1"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","","","30.6","39.1"]
["","","Ngrohje","I ulët","m³/min","18.9","24.8","27.2","28.3"]
["","Presioni i jashtëm statik","","Nom.","Pa","0","0","0","0"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","59","64","65","71"]
["","Ngrohje","","","dBA","62","64","65","71"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","49","52","52","56"]
["","","","Nom.","dBA","48","47"]
["","","","Mesatar","dBA","","","50","53"]
["","","","I ulët","dBA","46","46","49","46"]
["","Ngrohje","","I lartë","dBA","49","52","52","56"]
["","","","Mesatar","dBA","","","50","53"]
["","","","Nom.","dBA","48","47"]
["","","","I ulët","dBA","46","46","49","46"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","9.52","9.52","9.52","9.52"]
["","Gazi","","Dia. jasht.","mm","15.88","15.88","15.9","15.9"]
["","Kullimi","","","","19.05","19.05"]
["Sistemet e kontrollit","Telekomandë me rreze infra të kuqe","","","","ARCWLA","ARCWLA","ARCWLA","ARCWLA"]
["","Telekomandë me tela","","","","ARCWB","ARCWB"]
["Aksesore Standarde","Installation manual","","","","Installation manual","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","Wireless remote control"]
["","Battery","","","","Battery","Battery"]
["","Tubi i shkarkimit","","","","Drain pipe","Drain pipe"]
["","Screw for wireless remote","","","","Screw for wireless remote","Screw for wireless remote"]
["","Ferrite Core","","","","Ferrite Core","Ferrite Core"]
["","Installation manual (Ferrite Core)","","","","Installation manual (Ferrite Core)","Installation manual (Ferrite Core)"]
["","Outdoor wiring diagram","","","","Outdoor wiring diagram","Outdoor wiring diagram"]
["","Operation manual","","","","Operation manual","Operation manual"]
["","Drain hose","","","","Drain hose","Drain hose"]
["Furnizimi me energji","Faza","","","","1~","1~"]
["","Frekuenca","","","Hz","50","50"]
["","Tensioni","","","V","220-240","220-240"]