{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Niveli i presionit të zhurmës","Ngrohje","","Nom.","dBA","","49.0"]
["","Ftohje","","Nom.","dBA","","49.0"]
["Aksesore Standarde","Tapë kullimi","","","","","1"]
["","Manual instalimi","","","","","1"]
["","Etiketa e ngarkesës së ftohësit","","","","","1"]
["","Etiketa në shumë gjuhë për gazet e fluoruara të efektit serë","","","","","1"]
["","Masat e përgjithshme të sigurisë","","","","","1"]
["Antipiretik","Charge","","","TCO2Eq","","0.52"]
["","GWP","","","","","675"]
["","Ngarkesa","","","kg","","0.76"]
["","Lloji","","","","","R-32"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Maks.","°CDB","","50 (4), 46 (5)"]
["","","","Min.","°CDB","","-10"]
["Lidhjet e tubacioneve","Ndryshimi i nivelit","IU - OU","Maks.","m","","15"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","","0.02 (për gjatësinë e tubave që kalojnë 10m)"]
["Kompresori","Lloji","","","","","Kompresor me lëkundje i izoluar hermetikisht"]
["Dimensionet","Njësia","","Gjerësia","mm","","840"]
["","","","Thellësia","mm","","350"]
["","","","Height","mm","","552"]
["Pesha","Unit","","","kg","","32"]
["Power supply","Faza","","","","","1~"]
["","Frekuenca","","","Hz","","50"]
["","Tensioni","","","V","","220-240"]
["Shënime","","","","","(1) - E mundur vetëm në kombinim me ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Përmban gaze të fluorinuara të efektit serrë"]
["","","","","","(2) - E mundur vetëm në kombinim me ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Shiko skicën e veçantë për diapazonin e funksionimit"]
["","","","","","","(3) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]
["","","","","","","(4) - E mundur vetëm në kombinim me ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","","(5) - E mundur vetëm në kombinim me ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]
["Dimensionet","Njësia","","Lartësia","mm","552"]
["","","","Gjerësia","mm","840"]
["","","","Thellësia","mm","350"]
["Pesha","Njësia","","","kg","32"]
["Kompresori","Lloji","","","","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","-10"]
["","","","Maks.","°CDB","50 (4), 46 (5)"]
["Niveli i presionit të zhurmës","Ftohje","","Nom.","dBA","46.0"]
["","Ngrohje","","Nom.","dBA","47.0"]
["Agjenti ftohës","Mbushja","","","kg","0.76"]
["","Mbushja","","","tCO2Eq","0.52"]
["","GWP","","","","675"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","20"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 10m)"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","15"]
["Aksesore Standarde","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Furnizimi me energji","Frekuenca","","","Hz","50"]