{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":10,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L"]
[]
[]
[]
[]
["","","","","","ARXS50L2V1B","ARXS71L2V1B","ARXS25L2V1B (Archived)","ARXS35L2V1B (Archived)","ARXS60L2V1B (Archived)"]
["Niveli i presionit të zhurmës","Ngrohje","","I lartë","dBA","","","47","48"]
["","","","Nom.","dBA","","52","","","49"]
["","Ftohje","","I lartë","dBA","","","46","48"]
["","","","Nom.","dBA","","52","","","49"]
["Aksesore Standarde","Tapë kullimi","","","","","1","1","1","1"]
["","Manual instalimi","","","","","1","1","1","1"]
["Agjenti ftohës","Charge","","","TCO2Eq","","","2.1","2.5"]
["","GWP","","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","","1.70","1.0","1.2","1.50"]
["","Lloji","","","","","R-410A","R-410A","R-410A","R-410A"]
["Motori i ventilatorit","Shpejtësia","Ftohje","Super e ulët","rpm","","","780","780"]
["","","Ngrohje","Super e ulët","rpm","","","740","740"]
["Diapazoni i funksionimit","Ftohja","Ambienti","Maks.","°CDB","","46","46","46","46"]
["","","","Min.","°CDB","","-10","10","10","-10"]
["","Ngrohje","Ambienti","Maks.","°CWB","","18","18","18","18"]
["","","","Min.","°CWB","","-15","-15","-15","-15"]
["Lidhjet e tubacioneve","Ndryshimi i nivelit","IU - OU","Maks.","m","","20.0","15","15","20.0"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)"]
["Sound power level","Ftohje","","","dBA","","65","","","62"]
["","Ngrohje","","","dBA","","65","","","62"]
["Kompresori","Lloji","","","","","Kompresor me lëkundje i izoluar hermetikisht","Kompresor me lëkundje i izoluar hermetikisht","Kompresor me lëkundje i izoluar hermetikisht","Kompresor me lëkundje i izoluar hermetikisht"]
["Dimensionet","Njësia","","Gjerësia","mm","","825","765","765","825"]
["","","","Thellësia","mm","","300","285","285","300"]
["","","","Lartësia","mm","","735","550","550","735"]
["Pesha","Njësia","","","kg","","47","34","34","47"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ngrohje","Super e ulët","cfm","","","904","904"]
["","","","Super e ulët","m³/min","","","25.6","25.6"]
["","","Ftohje","Super e ulët","m³/min","","","30.1","30.1"]
["","","","Super e ulët","cfm","","","1,063","1,063"]
["Power supply","Faza","","","","","1~","1~","1~","1~"]
["","Frekuenca","","","Hz","","50","50","50","50"]
["","Tensioni","","","V","","220-230-240","220-240","220-240","220-230-240"]
["Shënime","","","","","(1) - 220V","","(1) - Kur lidhet me njësinë e jashtme të sistemeve të shumëfishta, referohuni specifikimeve të njësisë së jashtme të shumëfishtë për t'u lidhur.","(1) - Kur lidhet me njësinë e jashtme të sistemeve të shumëfishta, referohuni specifikimeve të njësisë së jashtme të shumëfishtë për t'u lidhur."]
["","","","","","(2) - 230V","","(2) - 220V","(2) - 220V"]
["","","","","","(3) - 240V","","(3) - 230V","(3) - 230V"]
["","","","","","","","(4) - 240V","(4) - 240V"]
["","","","","","","","(5) - Përmban gaze të fluorinuara të efektit serrë","(5) - Përmban gaze të fluorinuara të efektit serrë"]
["Ventilatori","Shkalla e qarkullimit të ajrit","Ftohje","Super e ulët","m³/min","48.9"]
["","","Ngrohje","Super e ulët","m³/min","43.1"]
["","","","Super e ulët","cfm","1727"]
["","","Ngrohje","Super e ulët","cfm","1522"]
["Dimensionet","Njësia","","Lartësia","mm","735"]
["","","","Gjerësia","mm","825"]
["","","","Thellësia","mm","300"]
["Pesha","Njësia","","","kg","47"]
["Motori i ventilatorit","Shpejtësia","Ftohje","Super e ulët","rpm","670"]
["","","Ngrohje","Super e ulët","rpm","670"]
["Kompresori","Lloji","","","","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","10"]
["","","","Maks.","°CDB","46"]
["","Ngrohje","Ambienti","Min.","°CWB","-15"]
["","","","Maks.","°CWB","18"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","48"]
["","Ngrohje","","I lartë","dBA","48"]
["Agjenti ftohës","Lloji","","","","R-410A"]
["","Mbushja","","","kg","1.7"]
["","Mbushja","","","tCO2Eq","3.5"]
["","GWP","","","","2087.5"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","30"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 10m)"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","20"]
["Aksesore Standarde","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["Furnizimi me energji","Faza","","","","1~"]
["","Frekuenca","","","Hz","50"]
["","Tensioni","","","V","220-240"]
["Aksesore Standarde","Etiketa në shumë gjuhë për gazet e fluoruara të efektit serë","","","","","1","1","","1"]
["","Etiketa e ngarkesës së ftohësit","","","","","1","1","","1"]
["Shënime","","","","","","(1) - Përmban gaze të fluorinuara të efektit serrë","","","(1) - Përmban gaze të fluorinuara të efektit serrë"]