{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":14,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A / ARXF-A"]
[]
[]
[]
[]
["","","","","ATXF20A5V1B / ARXF20A5V1B","ATXF25A5V1B / ARXF25A5V1B","ATXF35A5V1B / ARXF35A5V1B","ATXF50A2V1B / ARXF50A2V1B","ATXF50A2V1B / ARXF50A5V1B","ATXF50A2V1B / ARXF50A6V1B","ATXF60A2V1B / ARXF60A2V1B","ATXF60A2V1B / ARXF60A5V1B","ATXF71A2V1B / ARXF71A5V1B","ATXF71A2V1B / ARXF71A2V1B"]
["Outdoor unit","","","","ARXF20A5V1B","ARXF25A5V1B","ARXF35A5V1B"]
["Kapaciteti ftohës","Min.","","kW","1.3","1.3","1.3","1.7","1.70","1.70","1.70","1.70","2.30","2.30"]
["","Nom.","","kW","2.00","2.50","3.30","5","5.00","5.00","6.00","6.00","7.10","7.10"]
["","Maks.","","kW","2.6","3.0","3.8","6","6.00","6.00","7.00","7.00","7.30","7.30"]
["Kapaciteti ngrohës","Min.","","kW","1.30","1.30","1.30","1.7","1.70","1.70","1.70","1.70","2.30","2.30"]
["","Nom.","","kW","2.50","2.80","3.50","6","6.00","6.00","6.40","6.40","8.20","8.20"]
["","Maks.","","kW","3.50","4.00","4.80","7.7","7.70","7.70","8.00","8.00","9.00","9.00"]
["Efikasiteti nominal","EER","","","3.91","3.27","3.27","3.3","3.30","3.30","3.25","3.25","2.53","2.53"]
["","COP","","","4.16","3.98","3.98","3.71","3.71","3.71","3.90","3.90","3.12","3.12"]
["","Konsumi vjetor i energjisë","","kWh","","","","758","758","758","923","923","1403","1403"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A","A","A","A","A","A","A","A","E","E"]
["","","Ngrohje","","A","A","A","A","A","A","A","A","D","D"]
["Ftohja e hapësirës","Kategoria e efikasitetit të energjisë","","","A++","A++","A++","A++","A++","A++","A++","A++","A","A"]
["","Kapaciteti","Pdesign","kW","2.00","2.50","3.50","5","5.00","5.00","6.00","6.00","7.10","7.10"]
["","SEER","","","6.12","6.19","6.18","6.18","6.18","6.18","6.12","6.12","5.12","5.12"]
["","Konsumi vjetor i energjisë","","kWh/a","114","141","198","283","283","283","343","343","486","486"]
["Ngrohja e hapësirës (klimë mesatare)","Kategoria e efikasitetit të energjisë","","","A+","A+","A+","A+","A+","A+","A+","A+","A","A"]
["","Kapaciteti","Pdesign","kW","2.20","2.40","2.80","4.6","4.60","4.60","4.80","4.80","6.20","6.20"]
["","SCOP/A","","","4.07","4.03","4.03","4.03","4.03","4.03","4.03","4.03","3.81","3.81"]
["","Pdh Kapaciteti i ngrohjes në -10°","","kW","1.99","2.10","2.33","4.06","4.06","4.06","4.24","4.24","5.02","5.02"]
["","Konsumi vjetor i energjisë","","kWh/a","756","831","972","1598","1598","1598","1668","1668","2278","2278"]