{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":87,"n_cols":11,"rows_kept":87,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A"]
[]
[]
[]
[]
["","","","","","ATXF20A5V1B","ATXF25A5V1B","ATXF35A5V1B","ATXF50A2V1B","ATXF60A2V1B","ATXF71A2V1B"]
["Niveli i presionit të zhurmës","Ngrohje","","I lartë","dBA","40","","","42","44","45"]
["","","","Mesatar","dBA","34","","","38","40","41"]
["","","","Funksionim pa zhurmë","dBA","21","","","30","32","33"]
["","","","I ulët","dBA","28","","","33","35","36"]
["","Ftohje","","Mesatar","dBA","33","","","39","41","42"]
["","","","Funksionim pa zhurmë","dBA","20","","","31","33","34"]
["","","","I ulët","dBA","26","","","34","36","37"]
["","","","I lartë","dBA","40","","","43","45","46"]
["Aksesore Standarde","Bateri AAA me qeliza të thata","","","","2","","","2","2","2"]
["","Manual instalimi","","","","1","","","1","1","1"]
["","Manual përdorimi","","","","1","","","1","1","1"]
["","Telekomandë me rreze infra të kuqe","","","","1","","","1","1","1"]
["","Mbajtës telekomande","","","","1","","","1","1","1"]
["","Pllakë montimi","","","","1","","","1","1","1"]
["","Vida mbërthimi për njësinë e brendshme","","","","2","","","2","2","2"]
["Sisteme kontrolli","Wired remote control","","","","BRC944B2, BRC073A1","","","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","","","ARC470A1","ARC470A1","ARC470A1"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","6.35","","","6.35","6.35","6.35"]
["","Gazi","","Dia. jasht.","mm","9.50","","","12.7","12.7","12.7"]
["","Kullimi","","","","18","","","18","18","18"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","0.019","","","0.029","0.032","0.032"]
["","Ngrohje","","Nom.","kW","0.020","","","0.032","0.035","0.035"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","55","","","59","60","62"]
["","Ngrohje","","","dBA","55","","","61","62","62"]
["Dimensionet","Njësia","","Gjerësia","mm","770","","","990","990","990"]
["","","","Thellësia","mm","225","","","263","263","263"]
["","","","Lartësia","mm","286","","","295","295","295"]
["Veshja e jashtme","Colour","","","","E bardhë","","","E bardhë","E bardhë","E bardhë"]
["Pesha","Njësia","","","kg","8.50","","","13.5","13.5","13.5"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ngrohje","I lartë","m³/min","10.3","","","17.3","17.9","17.9"]
["","","","I ulët","m³/min","6.7","","","12.2","12.8","12.8"]
["","","","Mesatar","m³/min","8.6","","","14.8","15.8","15.8"]
["","","","Funksionim pa zhurmë","m³/min","5.3","","","10.7","11.3","11.3"]
["","","Ftohje","I ulët","m³/min","6.1","","","11.9","12.2","12.2"]
["","","","Mesatar","m³/min","8.1","","","14.4","14.8","14.8"]
["","","","I lartë","m³/min","10.1","","","16.8","17.3","17.3"]
["","","","Funksionim pa zhurmë","m³/min","4.4","","","10.5","10.7","10.7"]
["Power supply","Phase","","","","1~","","","1~","1~","1~"]
["","Frekuenca","","","Hz","50","","","50","50","50"]
["","Emri","","","","","","","V1","V1","V1"]
["","Tensioni","","","V","220-240","","","220-240","220-240","220-240"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","","0.019","0.032"]
["","Ngrohje","","Nom.","kW","","0.02","0.032"]
["Veshja e jashtme","Ngjyra","","","","","E bardhë","E bardhë"]
["Dimensionet","Njësia","","Lartësia","mm","","286","286"]
["","","","Gjerësia","mm","","770","770"]
["","","","Thellësia","mm","","225","225"]
["Pesha","Njësia","","","kg","","8.5","9"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","","10.1","11.5"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","","8.1","8.3"]
["","","","I ulët","m³/min","","6.1","6.3"]
["","","","Funksionim pa zhurmë","m³/min","","4.4","4.5"]
["","","Ngrohje","I lartë","m³/min","","10.3","11.5"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","","8.6","9"]
["","","Ngrohje","I ulët","m³/min","","6.7","7"]
["","","","Funksionim pa zhurmë","m³/min","","5.3","5.3"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","","55","58"]
["","Ngrohje","","","dBA","","55","58"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","","40","43"]
["","","","Mesatar","dBA","","33","34"]
["","","","I ulët","dBA","","26","27"]
["","","","Funksionim pa zhurmë","dBA","","20","20"]
["","Ngrohje","","I lartë","dBA","","40","40"]
["","","","Mesatar","dBA","","34","35"]
["","","","I ulët","dBA","","28","29"]
["","","","Funksionim pa zhurmë","dBA","","21","21"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","","6.35","6.35"]
["","Gazi","","Dia. jasht.","mm","","9.5","9.5"]
["","Kullimi","","","","","18","18"]
["Sistemet e kontrollit","Telekomandë me rreze infra të kuqe","","","","","ARC470A1","ARC470A1"]
["","Telekomandë me tela","","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Aksesore Standarde","Installation manual","","","","","1","1"]
["","AAA dry-cell batteries","","","","","2","2"]
["","Operation manual","","","","","1","1"]
["","Indoor unit fixing screws","","","","","2","2"]
["","Infrared remote control","","","","","1","1"]
["","Mounting plate","","","","","1","1"]
["","Remote control holder","","","","","1","1"]
["Furnizimi me energji","Faza","","","","","1~","1~"]
["","Frekuenca","","","Hz","","50","50"]
["","Tensioni","","","V","","220-240","220-240"]