{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-K3 / ARXP-K3"]
[]
[]
[]
[]
["","","","","ATXP20K3V1B / ARXP20K3V1B","ATXP25K3V1B / ARXP25K3V1B","ATXP35K3V1B / ARXP35K3V1B"]
["Kapaciteti ftohës","Nom.","","kW","","2.50","3.50"]
["Efikasiteti nominal","EER","","","","3.79","3.45"]
["","COP","","","","4.36","4.02"]
["","Direktiva e etiketimit të energjisë","Ftohje","","","A","A"]
["","","Ngrohje","","","A","A"]
["Kapaciteti ngrohës","Nom.","","kW","","3.00","4.00"]
["Shënime","","","","","(1) - Ftohje: T2: temp. brend. 26,6°CDB, 19,4°CWB, temp. e jasht. 48°CDB [Btu/hr/W]","(1) - Ftohje: T2: temp. brend. 26,6°CDB, 19,4°CWB, temp. e jasht. 48°CDB [Btu/hr/W]"]
["","","","","","(2) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m.","(2) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m."]
["","","","","","(3) - Shiko skicën e veçantë për të dhënat e skicave elektrike","(3) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]
["Outdoor unit","","","","ARXP20K3V1B"]
["Kapaciteti ftohës","Nom.","","kW","2.00"]
["Kapaciteti ngrohës","Nom.","","kW","2.50"]
["Efikasiteti nominal","EER","","","3.98"]
["","COP","","","4.77"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A"]
["","","Ngrohje","","A"]
["Ftohja e hapësirës","Kategoria e efikasitetit të energjisë","","","A++"]
["","Kapaciteti","Pdesign","kW","2.00"]
["","SEER","","","6.75"]
["","Konsumi vjetor i energjisë","","kWh/a","104"]
["Ngrohja e hapësirës (klimë mesatare)","Kategoria e efikasitetit të energjisë","","","A++"]
["","Kapaciteti","Pdesign","kW","2.20"]
["","SCOP/A","","","4.64"]
["","Pdh Kapaciteti i ngrohjes në -10°","","kW","2.19"]
["","Konsumi vjetor i energjisë","","kWh/a","664"]