{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":7,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-M"]
[]
[]
[]
[]
["","","","","","ATXP25M5V1B (Archived)","ATXP35M5V1B (Archived)"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","0.02","0.032"]
["","Ngrohje","","Nom.","kW","0.023","0.032"]
["Veshja e jashtme","Ngjyra","","","","E bardhë","E bardhë"]
["Dimensionet","Njësia","","Lartësia","mm","286","286"]
["","","","Gjerësia","mm","770","770"]
["","","","Thellësia","mm","225","225"]
["Pesha","Njësia","","","kg","8.5","9"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","9.7","11.5"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","7.7","8.3"]
["","","","I ulët","m³/min","5.8","6.3"]
["","","","Funksionim pa zhurmë","m³/min","4.2","4.5"]
["","","Ngrohje","I lartë","m³/min","10.4","11.5"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","8.1","9"]
["","","Ngrohje","I ulët","m³/min","6.4","7"]
["","","","Funksionim pa zhurmë","m³/min","5.2","5.3"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","55","58"]
["","Ngrohje","","","dBA","55","58"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","40","43"]
["","","","Mesatar","dBA","33","34"]
["","","","I ulët","dBA","26","27"]
["","","","Funksionim pa zhurmë","dBA","19","20"]
["","Ngrohje","","I lartë","dBA","40","40"]
["","","","Mesatar","dBA","34","35"]
["","","","I ulët","dBA","28","29"]
["","","","Funksionim pa zhurmë","dBA","21","21"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","6.35","6.35"]
["","Gazi","","Dia. jasht.","mm","9.5","9.5"]
["","Kullimi","","","","18","18"]
["Sistemet e kontrollit","Telekomandë me rreze infra të kuqe","","","","ARC480A53","ARC480A53"]
["","Telekomandë me tela","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Aksesore Standarde","Installation manual","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2"]
["","Indoor unit fixing screws","","","","2","2"]
["","Infrared remote control","","","","1","1"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Furnizimi me energji","Faza","","","","1~","1~"]
["","Frekuenca","","","Hz","50","50"]
["","Tensioni","","","V","220-240","220-240"]