{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":8,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-N9"]
[]
[]
[]
[]
["","","","","","ATXP20N5V1B9","ATXP25N5V1B9","ATXP35N5V1B9"]
["Power input","Ftohje","","Nom.","kW","0.019","0.020","0.032"]
["","Ngrohje","","Nom.","kW","0.023","0.023","0.032"]
["Veshja e jashtme","Colour","","","","E bardhë","E bardhë","E bardhë"]
["Dimensionet","Njësia","","Lartësia","mm","286","286","286"]
["","","","Gjerësia","mm","770","770","770"]
["","","","Thellësia","mm","225","225","225"]
["Pesha","Njësia","","","kg","8.50","8.50","9.00"]
["Ventilatori","Shkalla e qarkullimit të ajrit","Ftohje","I lartë","m³/min","9.5","9.7","11.5"]
["","","","Mesatar","m³/min","7.4","7.7","8.3"]
["","","","I ulët","m³/min","5.6","5.8","6.3"]
["","","","Funksionim pa zhurmë","m³/min","4.2","4.2","4.5"]
["","","Ngrohje","I lartë","m³/min","10.4","10.4","11.5"]
["","","","Mesatar","m³/min","8.1","8.1","9.0"]
["","","","I ulët","m³/min","6.2","6.4","7.0"]
["","","","Funksionim pa zhurmë","m³/min","5.2","5.2","5.1"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","55","55","58"]
["","Ngrohje","","","dBA","55","55","58"]
["Niveli i presionit të zhurmës","Ftohje","","I lartë","dBA","39","40","43"]
["","","","Mesatar","dBA","33","33","34"]
["","","","I ulët","dBA","25","26","27"]
["","","","Funksionim pa zhurmë","dBA","19","19","20"]
["","Ngrohje","","I lartë","dBA","39","40","40"]
["","","","Mesatar","dBA","34","34","35"]
["","","","I ulët","dBA","28","28","29"]
["","","","Funksionim pa zhurmë","dBA","21","21","21"]
["Piping connections","Lëngu","","Dia. jasht.","mm","6","6","6"]
["","Gas","","Dia. jasht.","mm","9.50","9.50","9.50"]
["","Kullimi","","","","18","18","18"]
["Control systems","Infrared remote control","","","","ARC480A78","ARC480A78","ARC480A78"]
["","Wired remote control","","","","BRC073A1","BRC073A1","BRC073A1"]
["Aksesore Standarde","Manual instalimi","","","","1","1","1"]
["","Manual përdorimi","","","","1","1","1"]
["","Telekomandë me rreze infra të kuqe","","","","1","1","1"]
["","Bateri AAA me qeliza të thata","","","","2","2","2"]
["","Mbajtës telekomande","","","","1","1","1"]
["","Pllakë montimi","","","","1","1","1"]
["","Filtër prej apatiti titani për largimin e aromave","","","","1","1","1"]
["","Filtri prej argjendi për grimcat","","","","1","1","1"]
["","Vida mbërthimi për njësinë e brendshme","","","","2","2","2"]
["","Masat e përgjithshme të sigurisë","","","","1","1","1"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Frekuenca","","","Hz","50","50","50"]
["","Tensioni","","","V","220-240","220-240","220-240"]
["Shënime","","","","","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 5m; diferenca e nivelit: 0m"]
["","","","","","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m (horizontal)","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m (horizontal)","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m (horizontal)"]
["","","","","","(3) - Shiko skicën e veçantë për të dhënat e skicave elektrike","(3) - Shiko skicën e veçantë për të dhënat e skicave elektrike","(3) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]