{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BEV2N-A"]
[]
[]
[]
[]
["","","","","BEV2N112A7V1B"]
["Niveli i presionit të zhurmës","Ngrohje","Në shpejtësi të lartë të ventilatorit","dBA","41"]
["","Ftohje","Në shpejtësi të lartë të ventilatorit","dBA","41"]
["Aksesore Standarde","Manual instalimi","","","1"]
["","Izolues për tubacionet","","","2"]
["","Fasheta lidhëse për kabllot","","","10"]
["Agjenti ftohës","GWP","","","1"]
["","Lloji","","","R744 (CO2)"]
["Lidhjet e tubacioneve","Lëngu","Dia. jasht.","mm","9.52"]
["","","Lloji","","Lidhje e kallajisur"]
["Dimensionet","Njësia","Gjerësia","mm","388"]
["","","Thellësia","mm","326"]
["","","Lartësia","mm","207"]
["Veshja e jashtme","Materiali","","","Fletë metalike e galvanizuar"]
["Pesha","Njësia","","kg","11"]
["Power supply","Faza","","","1~"]
["","Frekuenca","","Hz","50/60"]
["","Tensioni","","V","220-240/220"]