{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BR00000554"]
[]
[]
[]
[]
["","","","","","BR00000554."]
["Përdorimi","","","","","Lloj që qëndron në dysheme"]
["Kapaciteti","m³/min","","","","33.33"]
["Veshja e jashtme","Ngjyra","","","","Finiturë çeliku e lyer dhe e galvanizuar"]
["Dimensionet","Njësia","","Lartësia","mm","1628"]
["","","","Gjerësia","mm","720"]
["","","","Thellësia","mm","770"]
["Pesha","Njësia","","","kg","150"]
["Sipërfaqja e hapësirës së përdorur","m²","","","","133"]
["Funksioni për pastrimin e ajrit","Fuqia në hyrje","","H","kW","0.379"]
["Niveli i presionit të zhurmës","Funksioni për pastrimin e ajrit","","I lartë","dBA","55.9"]
["Ventilatori","Niveli i qarkullimit të ajrit","Funksioni për pastrimin e ajrit","Turbo","m³/h","2300"]
["","","","I lartë","m³/h","2000"]
["Metoda e grumbullimit të pluhurit","","","","","Parafiltër RedPleat, ISO i trashë 70% 592x592x45, Filtri H14 HEPA"]
["Pajisjet e sigurisë","Artikulli","","01","","Çelësi i sigurisë (puna ndalon kur hapet paneli i pasmë)"]
["Aksesore Standarde","Prefilter selected","","","","1"]
["","HEPA filter selected","","","","1"]
["","Quick Start and Maintenance Guide","","","","1"]
["","Installation and Operation Manual available for download","","","","1"]
["Kablloja elektrike","m","","","","3"]
["Furnizimi me energji","Frekuenca","","","Hz","50/60"]
["Rryma e funksionimit","Funksioni për pastrimin e ajrit","","I lartë","A","1.73"]