{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":13,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHVX-A / 5XXM-A"]
[]
[]
[]
[]
["","","","","","CHVX07S18AJ4V / 5XXM68A2V1B","CHVX07S18AJ9W / 5XXM68A2V1B","CHVX07S23AJ4V / 5XXM68A2V1B","CHVX07S23AJ9W / 5XXM68A2V1B","CHVX07S18AJ4V / 5XXM90A2V1B","CHVX07S18AJ9W / 5XXM90A2V1B","CHVX07S23AJ4V / 5XXM90A2V1B","CHVX07S23AJ9W / 5XXM90A2V1B"]
["Kapaciteti ngrohës","Nom.","","","kW","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)"]
["Kapaciteti ftohës","Nom.","","","kW","6.50 (1)","6.50 (1)","6.50 (1)","6.50 (1)","7.00 (1)","7.00 (1)","7.00 (1)","7.00 (1)"]
["Fuqia në hyrje","Ngrohje","","Nom.","kW","1.33 (1), 2.27 (2)","1.33 (1), 2.27 (2)","1.33 (1), 2.27 (2)","1.33 (1), 2.27 (2)","1.79 (1), 2.89 (2)","1.79 (1), 2.89 (2)","1.79 (1), 2.89 (2)","1.79 (1), 2.89 (2)"]
["","Ftohje","","Nom.","kW","1.80 (1)","1.80 (1)","1.80 (1)","1.80 (1)","1.94 (1)","1.94 (1)","1.94 (1)","1.94 (1)"]
["COP","","","","","4.50 (1), 2.60 (2)","4.50 (1), 2.60 (2)","4.50 (1), 2.60 (2)","4.50 (1), 2.60 (2)","4.20 (1), 2.70 (2)","4.20 (1), 2.70 (2)","4.20 (1), 2.70 (2)","4.20 (1), 2.70 (2)"]
["EER","","","","","3.61 (1)","3.61 (1)","3.61 (1)","3.61 (1)","3.61 (1)","3.61 (1)","3.61 (1)","3.61 (1)"]
["Ngrohje uji të ngrohtë shtëpiak","Të përgjithshme","","Profili i deklaruar i ngarkesës","","L","L","L","L","L","L","L","L"]
["","Klimë mesatare","","Kategoria e efikasitetit të energjisë të ngrohjes së ujit","","A+","A+","A+","A+","A+","A+","A+","A+"]
["Ngrohja e ambientit","Dalja e ujit për klimë mesatare 55°C","Të përgjithshme","SCOP","","3.00","3.00","3.00","3.00","3.00","3.00","3.00","3.00"]
["","Dalja e ujit klimë mesatare 55°C","Të përgjithshme","Klas. efikasitetit të ngrohjes sezonale të ambientit","","A+","A+","A+","A+","A+","A+","A+","A+"]
["","Dalja e ujit për klimë mesatare 35°C","Të përgjithshme","SCOP","","4.25","4.25","4.25","4.25","4.10","4.10","4.10","4.10"]
["","Dalja e ujit klimë mesatare 35°C","Të përgjithshme","Klas. efikasitetit të ngrohjes sezonale të ambientit","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Gama e efikasitetit të energjisë","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Shënime","","","","","(2) - Temperatura e hyrjes/daljes së ujit 7/12 °C; temperatura e hyrjes së ajrit 27°C DB 19°C WB.","(1) - Temperatura e hyrjes/daljes së ujit 7/12 °C; temperatura e hyrjes së ajrit 27°C DB 19°C WB.","(1) - Temperatura e hyrjes/daljes së ujit 7/12 °C; temperatura e hyrjes së ajrit 27°C DB 19°C WB.","(1) - Temperatura e hyrjes/daljes së ujit 7/12 °C; temperatura e hyrjes së ajrit 27°C DB 19°C WB.","(2) - Temperatura e hyrjes/daljes së ujit 7/12 °C; temperatura e hyrjes së ajrit 27°C DB 19°C WB.","(1) - Temperatura e hyrjes/daljes së ujit 7/12 °C; temperatura e hyrjes së ajrit 27°C DB 19°C WB.","(1) - Temperatura e hyrjes/daljes së ujit 7/12 °C; temperatura e hyrjes së ajrit 27°C DB 19°C WB.","(1) - Temperatura e hyrjes/daljes së ujit 7/12 °C; temperatura e hyrjes së ajrit 27°C DB 19°C WB."]