{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":9,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32 / 5MXM-N"]
[]
[]
[]
[]
["","","","","","CHYHBH05AAV32 / 5MXM90N2V1B","CHYHBH08AAV32 / 5MXM90N2V1B","CHYHBH05AFV32 / 5MXM90N2V1B","CHYHBH08AFV32 / 5MXM90N2V1B"]
["Ngrohje e ujit të ngrohtë në shtëpi","Të përgjithshme","","Profili i deklaruar i ngarkesës","","XL","XL"]
["","Klimë mesatare","","Kategoria e efikasitetit të energjisë të ngrohjes së ujit","","A","A"]
["COP","","","","","4.04 (1)","4.17 (1)","4.04","4.17"]
["Ngrohja e ambientit","Dalja e ujit për klimë mesatare 55°C","Të përgjithshme","Seasonal space heating eff. class","","A+","A+"]
["","","","ηs (Efikasiteti sezonal i ngrohjes së ambientit)","%","120.8","120.8"]
["","","","SCOP","","3.09","3.09"]
["Kapaciteti ngrohës","Nom.","","","kW","4.50 (1)","6.78 (1)"]
["Shënime","","","","","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), duke shmangur bojlerin","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), duke shmangur bojlerin","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), duke shmangur bojlerin","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), duke shmangur bojlerin"]
["Kapaciteti ngrohës","Nom.","","","kW","","","4.5","6.78"]
["Ngrohje uji të ngrohtë shtëpiak","Të përgjithshme","","Profili i deklaruar i ngarkesës","","","","XL","XL"]
["","Klimë mesatare","","Kategoria e efikasitetit të energjisë të ngrohjes së ujit","","","","A","A"]
["Ngrohja e ambientit","Dalja e ujit për klimë mesatare 55°C","Të përgjithshme","SCOP","","","","3.09","3.09"]
["","Dalja e ujit klimë mesatare 55°C","Të përgjithshme","Klas. efikasitetit të ngrohjes sezonale të ambientit","","","","A+","A+"]