{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Niveli i presionit të zhurmës","Ngrohje","","I lartë","dBA","38","","41"]
["","","","Funksionim pa zhurmë","dBA","21","","21"]
["","","","I ulët","dBA","28","","30"]
["","Ftohje","","Funksionim pa zhurmë","dBA","21","","21"]
["","","","I ulët","dBA","25","","28"]
["","","","I lartë","dBA","37","","42"]
["","","","Nom.","dBA","33"]
["","Ftohje","","Nom.","dBA","31","","35"]
["Aksesore Standarde","Manual instalimi","","","","1","","1"]
["","Manual përdorimi","","","","1","","1"]
["","Telekomandë me valë","","","","1","","1"]
["","Bateri","","","","2","","2"]
["","Mbajtës telekomande","","","","1","","1"]
["","Pllakë montimi","","","","1","","1"]
["","Vida mbërthimi për njësinë e brendshme","","","","2","","2"]
["","Filtër fotokatalitik me apatit titani për pastrimin e ajrit","","","","2","","2"]
["Sistemet e kontrollit","Infrared remote control","","","","ARC466A6","","ARC466A6"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","6.35","","6.35"]
["","Gazi","","Dia. jasht.","mm","9.5","","9.5"]
["","Kullimi","","","","18","","18"]
["Power input","Ftohje","","Nom.","kW","0.040","","0.040"]
["","Ngrohje","","Nom.","kW","0.040","","0.040"]
["Sound power level","Ftohje","","","dBA","55","","59"]
["","Ngrohje","","","dBA","56","","58"]
["Dimensionet","Njësia","","Gjerësia","mm","780","","780"]
["","","","Thellësia","mm","215","","215"]
["","","","Lartësia","mm","289","","289"]
["Veshja e jashtme","Ngjyra","","","","E bardhë","","E bardhë"]
["Pesha","Njësia","","","kg","8","","8"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ngrohje","I lartë","m³/min","","","10.1"]
["","","","I ulët","m³/min","","","6.3"]
["","","","Funksionim pa zhurmë","m³/min","","","4.3"]
["","","Ftohje","I ulët","m³/min","","","5.2"]
["","","","I lartë","m³/min","","","9.2"]
["","","","Funksionim pa zhurmë","m³/min","","","3.9"]
["","","","Nom.","m³/min","","","8.1"]
["","","Ftohje","Nom.","m³/min","","","7.2"]
["Power supply","Faza","","","","1~","","1~"]
["","Frekuenca","","","Hz","50","","50"]
["","Emri","","","","V1","","V1"]
["","Tensioni","","","V","220-240","","220-240"]
["Shënime","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","","0.04","","0.040"]
["","Ngrohje","","Nom.","kW","","0.04","","0.040"]
["Veshja e jashtme","Ngjyra","","","","","E bardhë","","E bardhë"]
["Dimensionet","Njësia","","Lartësia","mm","","289","","289"]
["","","","Gjerësia","mm","","780","","780"]
["","","","Thellësia","mm","","215","","215"]
["Pesha","Njësia","","","kg","","8","","8.00"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","","7.9","","9.2"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","","6.3","","7.2"]
["","","","I ulët","m³/min","","4.7","","5.2"]
["","","","Funksionim pa zhurmë","m³/min","","3.9","","3.9"]
["","","Ngrohje","I lartë","m³/min","","9","","10.1"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","","7.5","","8.1"]
["","","Ngrohje","I ulët","m³/min","","6","","6.3"]
["","","","Funksionim pa zhurmë","m³/min","","4.3","","4.3"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","","55","","59"]
["","Ngrohje","","","dBA","","56","","58"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","","37","","42"]
["","","","Mesatar","dBA","","31","","35"]
["","","","I ulët","dBA","","25","","28"]
["","","","Funksionim pa zhurmë","dBA","","21","","21"]
["","Ngrohje","","I lartë","dBA","","38","","41"]
["","","","Mesatar","dBA","","33","","36"]
["","","","I ulët","dBA","","28","","30"]
["","","","Funksionim pa zhurmë","dBA","","21","","21"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","","6.35","","6.35"]
["","Gazi","","Dia. jasht.","mm","","9.5","","9.50"]
["","Kullimi","","","","","18","","18"]
["Sistemet e kontrollit","Infrared remote control","","","","","ARC466A6","","ARC466A6"]
["Aksesore Standarde","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["Furnizimi me energji","Emri","","","","","V1","","V1"]
["","Faza","","","","","1~","","1~"]
["","Frekuenca","","","Hz","","50","","50"]
["","Tensioni","","","V","","220-240","","220-240"]