{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["Fuqia në hyrje","kW","","","","0.015"]
["Numri maksimal i njësive të brendshme që lidhen","","","","","32"]
["Numri maksimal i njësive të jashtme që lidhen @","","","","","7"]
["Dimensionet","Njësia","","Lartësia","mm","136"]
["","","","Gjerësia","mm","384"]
["","","","Thellësia","mm","92"]
["Komunikimi","DIII-NET","","Sasia","","1"]
["","","","Shënime","","DIII-NET (F1F2)"]
["","Eternet","","Sasia","","1"]
["","Terminali i hyrjes","Dixhital","Sasia","","4"]
["Temperatura e ambientit","Funksionimi","","Min.","°C","-10"]
["","","","Maks.","°C","50"]
["","Ruajtja","","Min.","°C","-20"]
["","","","Maks.","°C","60"]
["","Temperatura e ambientit-=-Lagështia relative <-=-%","","","%","85"]
["Furnizimi me energji","Frekuenca","","","Hz","50/60"]
["","Tensioni","","","V","110-240 AC"]
["Shënime","","","","","(1) - Përfshin hyrjen e fuqisë së furnizimit me energji WAGO, modulin CPU dhe modulin I/O"]
["","","","","","(2) - Dimensionet përfshijnë furnizimin me energji WAGO, modulin CPU, modulin I/O dhe hapësirën e nevojshme mes pjesëve të ndryshme"]
["","","","","","(3) - Përmasat në ekranin opsional janë: lartësia: 209 mm, gjerësia: 123 mm, thellësia: 8,5 mm"]