{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":11,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EABX-D9W / EPGA011-016DV"]
[]
[]
[]
[]
["","","","","","EABX16DA9W / EPGA11DAV3","EABX16DF9W / EPGA11DAV3","EABX16DA9W / EPGA14DAV3","EABX16DF9W / EPGA14DAV3","EABX16DA9W / EPGA16DAV3","EABX16DF9W / EPGA16DAV3"]
["COP","","","","","5.15 (1), 3.88 (2)","5.15 (1), 3.88 (2)","4.99 (1), 3.65 (2)","4.99 (1), 3.65 (2)","4.78 (1), 3.71 (2)","4.78 (1), 3.71 (2)"]
["Njësia e brendshme","","","","","EABX16DA9W","EABX16DA9W","EABX16DA9W","EABX16DA9W","EABX16DA9W","EABX16DA9W"]
["Ngrohja e ambientit","Dalja e ujit për klimë mesatare 55°C","Të përgjithshme","Seasonal space heating eff. class","","A++","","A++","","A++"]
["","","","SCOP","","3.32","","3.37","","3.43"]
["","Dalja e ujit klimë mesatare 35°C","Të përgjithshme","Klas. efikasitetit të ngrohjes sezonale të ambientit","","A+++","","A+++","","A+++"]
["","","","SCOP","","4.44","","4.51","","4.61"]
["Kapaciteti ftohës","Nom.","","","kW","10.5 (1), 10.7 (2)","","11.1 (1), 11.9 (2)","","13.5 (1), 11.9 (2)"]
["EER","","","","","4.75 (1), 3.23 (2)","4.75 (1), 3.23 (2)","4.09 (1), 2.99 (2)","4.09 (1), 2.99 (2)","3.94 (1), 2.99 (2)","3.94 (1), 2.99 (2)"]
["Kapaciteti ngrohës","Nom.","","","kW","11.1 (1), 11.3 (2)","","14.5 (1), 14.5 (2)","","16.5 (1), 15.6 (2)"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","2.21 (1), 3.30 (2)","","2.72 (1), 3.97 (2)","","3.42 (1), 3.97 (2)"]
["","Ngrohje","","Nom.","kW","2.16 (1), 2.91 (2)","","2.91 (1), 3.96 (2)","","3.45 (1), 4.21 (2)"]
["Shënime","","","","","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]
["Kapaciteti ngrohës","Nom.","","","kW","","11.1 (1), 11.3 (2)","","14.5 (2) (1), 14.5 (2) (1)","","16.5 (1), 15.6 (2)"]
["Kapaciteti ftohës","Nom.","","","kW","","10.5 (1), 10.7 (2)","","11.1 (1), 11.9 (2)","","13.5 (1), 11.9 (2)"]
["Fuqia në hyrje","Ngrohje","","Nom.","kW","","2.16 (1), 2.91 (2)","","2.91 (1), 3.96 (2)","","3.45 (1), 4.21 (2)"]
["","Ftohje","","Nom.","kW","","2.21 (1), 3.30 (2)","","2.72 (1), 3.97 (2)","","3.42 (1), 3.97 (2)"]
["Ngrohja e ambientit","Dalja e ujit për klimë mesatare 55°C","Të përgjithshme","SCOP","","","3.32","","3.37","","3.43"]
["","Dalja e ujit klimë mesatare 55°C","Të përgjithshme","Klas. efikasitetit të ngrohjes sezonale të ambientit","","","A++","","A++","","A++"]
["","Dalja e ujit për klimë mesatare 35°C","Të përgjithshme","SCOP","","","4.44","","4.51","","4.61"]
["","Dalja e ujit klimë mesatare 35°C","Të përgjithshme","Klas. efikasitetit të ngrohjes sezonale të ambientit","","","A+++","","A+++","","A+++"]
["Gama e efikasitetit të energjisë","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","","Space Heating A+++ ~ D, Water Heating A+ ~ F","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]