{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":10,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EAVH-D6V / EPGA011-016DV"]
[]
[]
[]
[]
["","","","","EAVH16S18DA6V / EPGA11DAV3","EAVH16S23DA6V / EPGA11DAV3","EAVH16S18DA6V / EPGA14DAV3","EAVH16S23DA6V / EPGA14DAV3","EAVH16S18DA6V / EPGA16DAV3","EAVH16S23DA6V / EPGA16DAV3"]
["Ngrohje e ujit të ngrohtë në shtëpi","Të përgjithshme","Profili i deklaruar i ngarkesës","","L","XL","L","XL","L","XL"]
["","Klimë mesatare","Kategoria e efikasitetit të energjisë të ngrohjes së ujit","","A","A","A","A","A","A"]
["COP","","","","5.15 (1), 3.88 (2)","5.15 (1), 3.88 (2)","4.99 (1), 3.65 (2)","4.99 (1), 3.65 (2)","4.78 (1), 3.71 (2)","4.78 (1), 3.71 (2)"]
["Njësia e brendshme","","","","EAVH16S18DA6V","EAVH16S23DA6V","EAVH16S18DA6V","EAVH16S23DA6V","EAVH16S18DA6V","EAVH16S23DA6V"]
["Kapaciteti ngrohës","Nom.","","kW","11.1 (1), 11.3 (2)","11.1 (1), 11.3 (2)","14.5 (1), 14.5 (2)","14.5 (1), 14.5 (2)","16.5 (1), 15.6 (2)","16.5 (1), 15.6 (2)"]
["Fuqia në hyrje","Ngrohje","Nom.","kW","2.16 (1), 2.91 (2)","2.16 (1), 2.91 (2)","2.91 (1), 3.96 (2)","2.91 (1), 3.96 (2)","3.45 (1), 4.21 (2)","3.45 (1), 4.21 (2)"]
["Shënime","","","","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]