{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":15,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSH-E / ERGA04-08EVA"]
[]
[]
[]
[]
["","","","","","EHSH04P30EF / ERGA04EAV3A","EHSH04P30EG / ERGA04EAV3A","EHSH08P30EF / ERGA06EAV3A","EHSH08P50EF / ERGA06EAV3A","EHSH08P50EG / ERGA06EAV3A","EHSH08P30EG / ERGA06EAV3A","EHSH08P30EF / ERGA08EAV3A","EHSH08P50EF / ERGA08EAV3A","EHSH08P50EG / ERGA08EAV3A","EHSH08P30EG / ERGA08EAV3A"]
["Indoor unit","","","","","EHSH04P30EF","EHSH04P30EG","EHSH08P30EF","EHSH08P50EF","EHSH08P50EG","EHSH08P30EG","EHSH08P30EF","EHSH08P50EF","EHSH08P50EG","EHSH08P30EG"]
["Kapaciteti ngrohës","Nom.","","","kW","4.30 (1), 4.60 (2)","4.30 (1), 4.60 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)"]
["Fuqia në hyrje","Ngrohje","","Nom.","kW","0.840 (1), 1.26 (2)","0.840 (1), 1.26 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)"]
["COP","","","","","5.10 (1), 3.65 (2)","5.10 (1), 3.65 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)"]
["Ngrohje uji të ngrohtë shtëpiak","Të përgjithshme","","Profili i deklaruar i ngarkesës","","L","L","L","XL","XL","L","L","XL","XL","L"]
["","Klimë mesatare","","Kategoria e efikasitetit të energjisë të ngrohjes së ujit","","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["Ngrohja e ambientit","Dalja e ujit për klimë mesatare 55°C","Të përgjithshme","SCOP","","3.26","3.26","3.25","3.25","3.25","3.25","3.27","3.27","3.27","3.27"]
["","Dalja e ujit klimë mesatare 55°C","Të përgjithshme","Klas. efikasitetit të ngrohjes sezonale të ambientit","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Dalja e ujit për klimë mesatare 35°C","Të përgjithshme","SCOP","","4.48","4.48","4.47","4.47","4.47","4.47","4.56","4.56","4.56","4.56"]
["","Dalja e ujit klimë mesatare 35°C","Të përgjithshme","Klas. efikasitetit të ngrohjes sezonale të ambientit","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Shënime","","","","","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]
["Gama e efikasitetit të energjisë","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]