{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":9,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-E"]
[]
[]
[]
[]
["","","","","","EHSX04P30EF","EHSX04P50EF","EHSX08P30EF","EHSX08P50EF"]
["Veshja e jashtme","Ngjyra","","","","E bardhë (RAL9016) / E zezë (RAL9017)","E bardhë (RAL9016) / E zezë (RAL9017)","E bardhë (RAL9016) / E zezë (RAL9017)","E bardhë (RAL9016) / E zezë (RAL9017)"]
["","Materiali","","","","Polipropilen rezistent ndaj goditjeve","Polipropilen rezistent ndaj goditjeve","Polipropilen rezistent ndaj goditjeve","Polipropilen rezistent ndaj goditjeve"]
["Dimensionet","Njësia","","Lartësia","mm","1,892","1,905","1,892","1,905"]
["","","","Gjerësia","mm","594","792","594","792"]
["","","","Thellësia","mm","644","812","644","812"]
["Pesha","Njësia","","","kg","77","107","77","107"]
["PED","Kategoria","","","","Art. 4.3","Art. 4.3","Art. 4.3","Art. 4.3"]
["Agjenti ftohës","Lloji","","","","R-32","R-32","R-32","R-32"]
["","GWP","","","","675","675","675","675"]
["","Mbushja","","","kg","1.5","1.5","1.5","1.5"]
["Niveli i fuqisë së zhurmës","Nom.","","","dBA","39","39","39","39"]
["Diapazoni i funksionimit","Ngrohje","Ana e ujit","Min.","°C","18","18","18","18"]
["","","","Maks.","°C","65","65","65","65"]
["","Ftohje","Ambienti","Min.","°CDB","10","10","10","10"]
["","","Ana e ujit","Min.","°C","5","5","5","5"]
["","","","Maks.","°C","22","22","22","22"]
["Furnizimi me energji","Faza","","","","1~","1~","1~","1~"]
["","Frekuenca","","","Hz","50","50","50","50"]
["","Tensioni","","","V","230","230","230","230"]
["Shënime","","","","","(1) - Humbja e nxehtësisë sipas EN12897","(1) - Humbja e nxehtësisë sipas EN12897","(1) - Humbja e nxehtësisë sipas EN12897","(1) - Humbja e nxehtësisë sipas EN12897"]