{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":7,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSXB-D3 / ERGA-EV"]
[]
[]
[]
[]
["","","","","","EHSXB04P30DA3 / ERGA04EAV3","EHSXB04P50DA3 / ERGA04EAV3"]
["Ngrohje e ujit të ngrohtë në shtëpi","Të përgjithshme","","Profili i deklaruar i ngarkesës","","L","XL"]
["","Klimë mesatare","","Kategoria e efikasitetit të energjisë të ngrohjes së ujit","","A+","A"]
["COP","","","","","5.10 (1), 3.65 (2)","5.10 (1), 3.65 (2)"]
["Indoor unit","","","","","EHSXB04P30DA3","EHSXB04P50DA3"]
["Ngrohja e ambientit","Dalja e ujit klimë mesatare 55°C","Të përgjithshme","Seasonal space heating eff. class","","A++","A++"]
["","","","ηs (Efikasiteti sezonal i ngrohjes së ambientit)","%","129","129"]
["","","","SCOP","","3.29","3.29"]
["Kapaciteti ftohës","Nom.","","","kW","4.86 (1), 4.52 (2)","4.86 (1), 4.52 (2)"]
["EER","","","","","5.98 (1), 3.32 (2)","5.98 (1), 3.32 (2)"]
["Kapaciteti ngrohës","Nom.","","","kW","4.30 (1), 4.60 (2)","4.30 (1), 4.60 (2)"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","0.810 (1), 1.36 (2)","0.810 (1), 1.36 (2)"]
["","Ngrohje","","Nom.","kW","0.840 (1), 1.26 (2)","0.840 (1), 1.26 (2)"]
["Shënime","","","","","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]