{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":9,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-E9W / ERGA-EVH"]
[]
[]
[]
[]
["","","","","","EHVX08S18EA9W / ERGA06EAV3H","EHVX08S18EJ9W / ERGA06EAV3H","EHVX08S23EJ9W / ERGA06EAV3H","EHVX08S23EA9W / ERGA06EAV3H"]
["Kapaciteti ngrohës","Nom.","","","kW","6.0 (1), 5.9 (2)","6.0 (1), 5.9 (2)","6.0 (1), 5.9 (2)","6.00 (1), 5.90 (2)"]
["Kapaciteti ftohës","Nom.","","","kW","5.96 (1), 5.09 (2)","5.96 (1), 5.09 (2)","5.96 (1), 5.09 (2)","5.96 (1), 5.09 (2)"]
["Fuqia në hyrje","Ngrohje","","Nom.","kW","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)"]
["","Ftohje","","Nom.","kW","1.06 (1), 1.55 (2)","1.06 (1), 1.55 (2)","1.06 (1), 1.55 (2)","1.06 (1), 1.55 (2)"]
["","Uji i ngrohtë shtëpiak nga 10°C në 50°C","","Nom.","kWh","2.48","2.48","3.01","3.01"]
["Koha e ngrohjes nga 10°C në 50°C","orë","","","","1 orë 28 min","1 orë 28 min","1 orë 40 min","1 orë 40 min"]
["COP","","","","","4.85 (1), 3.5 (2)","4.85 (1), 3.5 (2)","4.85 (1), 3.5 (2)","4.85 (1), 3.50 (2)"]
["EER","","","","","5.61 (1), 3.28 (2)","5.61 (1), 3.28 (2)","5.61 (1), 3.28 (2)","5.61 (1), 3.28 (2)"]
["Ngrohje uji të ngrohtë shtëpiak","Të përgjithshme","","Profili i deklaruar i ngarkesës","","L","L","XL","XL"]
["","Klimë mesatare","","Kategoria e efikasitetit të energjisë të ngrohjes së ujit","","A+","A+","A+","A+"]
["Ngrohja e ambientit","Dalja e ujit për klimë mesatare 55°C","Të përgjithshme","SCOP","","3.28","3.28","3.28","3.28"]
["","Dalja e ujit klimë mesatare 55°C","Të përgjithshme","Klas. efikasitetit të ngrohjes sezonale të ambientit","","A++","A++","A++","A++"]
["","Dalja e ujit për klimë mesatare 35°C","Të përgjithshme","SCOP","","4.52","4.52","4.52","4.52"]
["","Dalja e ujit klimë mesatare 35°C","Të përgjithshme","Klas. efikasitetit të ngrohjes sezonale të ambientit","","A+++","A+++","A+++","A+++"]
["Shënime","","","","","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]
["Energy Efficiency Range","","","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]