{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":7,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWET-BV3"]
[]
[]
[]
[]
["","","","","","EKHWET90BAV3","EKHWET120BAV3"]
["Montimi","","","","","Mur","Mur"]
["Veshja e jashtme","Ngjyra","","","","Bardhezi","Bardhezi"]
["","Materiali","","","","Fletë metalike, Akrilonitril butadien stiren","Fletë metalike, Akrilonitril butadien stiren"]
["Dimensionet","Njësia","Lartësia","Rezervuari","mm","1032","1283"]
["","","","Gjerësia","mm","510","510"]
["","","","Thellësia","mm","570","570"]
["Pesha","Njësia","","Bosh","kg","43","47"]
["Rezervuari","Vëllimi i ujit","","","l","89","118"]
["","Materiali","","","","Çelik i veshur me emal sipas DIN4753TL2","Çelik i veshur me emal sipas DIN4753TL2"]
["Depozita","Temperatura maksimale e ujit","","","°C","75.0","75.0"]
["","Kategoria e efikasitetit të energjisë","","","","B","C"]
["Shkëmbyesi i nxehtësisë","Ujë i ngrohtë në shtëpi","","Sasia","","1","1"]
["","","","Materiali i tubit","","Alumin","Alumin"]
["","","","Presioni i funksionimit","bar","42","42"]
["Ngrohësi përforcues","Kapaciteti","","","kW","1.2","1.2"]
["Gama e efikasitetit të energjisë","","","","","A+ ~ F","A+ ~ F"]