{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":8,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWP-B"]
[]
[]
[]
[]
["","","","","","EKHWP300B","EKHWP54419BA","EKHWP500B"]
["Shkëmbyesi i nxehtësisë","Ngarkesa","","Sasia","","","1"]
["","","","Presioni i funksionimit","bar","","3.0"]
["","","","Materiali i tubit","","","Inoks (DIN 1.4404)"]
["","","","Vëllimi i bobinës së brendshme","l","","10.0"]
["","Ujë i ngrohtë në shtëpi","","Materiali i tubit","","","Inoks (DIN 1.4404)"]
["","","","Presioni i funksionimit","bar","","10.0"]
["","","","Vëllimi i bobinës së brendshme","l","","28.9"]
["","","","Sasia","","","1"]
["","Ngrohja ndihmëse e panelit diellor","","Vëllimi i bobinës së brendshme","l","","3.9"]
["","","","Presioni i funksionimit","bar","","3.0"]
["","","","Materiali i tubit","","","Inoks (DIN 1.4404)"]
["","","","Sasia","","","1"]
["Dimensionet","Unit","","Width","mm","","790"]
["","","Lartësia","Rezervuari","mm","","1,658"]
["","","","Thellësia","mm","","790"]
["Veshja e jashtme","Materiali","","","","","Polipropilen rezistent ndaj goditjeve"]
["","Ngjyra","","","","","E bardhë trafiku (RAL9016) / Gri e errët (RAL7011)"]
["Depozita","Kategoria e efikasitetit të energjisë","","","","","B"]
["","Temperatura maksimale e ujit","","","°C","","85"]
["","Materiali","","","","","Polipropilen"]
["","Vëllimi i ujit","","","l","","477"]
["Pesha","Njësia","","Bosh","kg","","71"]
["","","","E plotë","kg","","548"]
["Montimi","","","","","","Në dysheme"]
["Shënime","","","","","(1) - Humbja e nxehtësisë sipas EN12897","(1) - Humbja e nxehtësisë sipas EN12897","(1) - Humbja e nxehtësisë sipas EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃"]
["","","","","","(5) - Për volumin në rubinet 140l -> 5820 Wh (banjë) / 8kW pompë ngrohëse","(5) - Për volumin në rubinet 140l -> 5820 Wh (banjë) / 8kW pompë ngrohëse","(5) - Për volumin në rubinet 140l -> 5820 Wh (banjë) / 16kW pompë ngrohëse"]
["","","","","","(6) - Për volumin në rubinet 90l -> 3660 Wh (banjë) / 8kW pompë ngrohëse","(6) - Për volumin në rubinet 90l -> 3660 Wh (banjë) / 8kW pompë ngrohëse","(6) - Për volumin në rubinet 90l -> 3660 Wh (banjë) / 16kW pompë ngrohëse"]
["","","","","","","(7) - Për volumin në rubinet 140l -> 5820 Wh (banjë) / 16kW pompë ngrohëse"]
["","","","","","","(8) - Për volumin në rubinet 90l -> 3660 Wh (banjë) / 16kW pompë ngrohëse"]
["","","","","","","(9) - Shkëmbyesi i nxehtësisë i lidhur në paralel, TKW= 10°C/ TWW= 45°C/ TSP= 65°C/ Pload= 35 kW/ Tflow= 80°C"]
["","","","","","","(10) - TKW= 10°C/ TWW= 45°C/ TSP= 65°C/ Pload= 35 kW/ Tflow= 80°C"]
["Montimi","","","","","Në dysheme","","Në dysheme"]
["Veshja e jashtme","Ngjyra","","","","E bardhë trafiku (RAL9016) / Gri e errët (RAL7011)","","E bardhë trafiku (RAL9016) / Gri e errët (RAL7011)"]
["","Materiali","","","","Polipropilen rezistent ndaj goditjeve","","Polipropilen rezistent ndaj goditjeve"]
["Dimensionet","Njësia","Lartësia","Rezervuari","mm","1646","","1658"]
["","","","Gjerësia","mm","595","","790"]
["","","","Thellësia","mm","615","","790"]
["Pesha","Njësia","","Bosh","kg","53","","76"]
["","","","E plotë","kg","347","","553"]
["Rezervuari","Vëllimi i ujit","","","l","294","","477"]
["","Materiali","","","","Polipropilen","","Polipropilen"]
["Depozita","Temperatura maksimale e ujit","","","°C","85","","85"]
["","Kategoria e efikasitetit të energjisë","","","","B","","B"]
["Shkëmbyesi i nxehtësisë","Ujë i ngrohtë në shtëpi","","Sasia","","1","","1"]
["","","","Materiali i tubit","","Çelik inoks (DIN 1.4404)","","Çelik inoks (DIN 1.4404)"]
["","","","Vëllimi i bobinës së brendshme","l","27.8","","28.9"]
["","","","Presioni i funksionimit","bar","10.0","","10.0"]
["","Ngarkesa","","Sasia","","1","","1"]
["","","","Materiali i tubit","","Çelik inoks (DIN 1.4404)","","Çelik inoks (DIN 1.4404)"]
["","","","Vëllimi i bobinës së brendshme","l","12.9","","18.1"]
["","","","Presioni i funksionimit","bar","6.0","","6.0"]
["","Ngrohja ndihmëse e panelit diellor","","Sasia","","","","1"]
["","","","Materiali i tubit","","","","Çelik inoks (DIN 1.4404)"]
["","","","Vëllimi i bobinës së brendshme","l","","","3.9"]
["","","","Presioni i funksionimit","bar","","","3.0"]