{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKSH-P"]
[]
[]
[]
[]
["","","","","EKSH26P1","EKSH26P"]
["Përthithësi","","","","Grumbullues me tuba bakri në formë harpe me pllakë të veçantë alumini të veshur dhe të ngjitur me laser","Grumbullues me tuba bakri në formë harpe me pllakë të veçantë alumini të veshur dhe të ngjitur me laser"]
["Temperatura në gjendje pushimi","Maks.","","°C","192","192"]
["Dimensionet","Njësia","Gjerësia","mm","2,000","85"]
["","","Thellësia","mm","85","1,300"]
["","","Lartësia","mm","1,300","2,000"]
["Presioni i funksionimit","Maks.","","bar","6","6"]
["Pesha","Njësia","","kg","42","42"]
["Sipërfaqja","Sipërfaqja e hapjes","","m² (2)","2.360","2.360"]
["","Përthithësi","","m² (2)","2.36","2.35"]
["","E jashtme","","m² (2)","2.60","2.60"]
["Montimi","","","","Horizontal","Horizontal"]
["Veshja me xham","","","","Xham sigurie me një fletë, transmetimi +/- 92%","Xham sigurie me një fletë, transmetimi +/- 92%"]
["Këndi i lejuar i çatisë","Maks.","","°","80","80"]
["","Min.","","°","15","15"]
["Veshja","","","","Mikro-term (përthithja maks. 96%, emetimi rreth 5% +/-2%)","Mikro-term (përthithja maks. 96%, emetimi rreth 5% +/-2%)"]
["Vëllimi","l","","","2.1","2.1"]
["Performanca termike","Efikasiteti pa humbje η0","","%","0.710","0.784"]
["","Koeficienti i humbjes së nxehtësisë a1","","W/m².K","4.300","4.250"]
["","Varësia e temperaturës e koeficientit të humbjes së energjisë a2","","W/m².K²","0.006","0.007"]
["","Kapaciteti termik","","kJ/K","6.5","6.5"]