{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EVH"]
[]
[]
[]
[]
["","","","","","ERGA06EAV3H"]
["Dimensionet","Njësia","","Lartësia","mm","740"]
["","","","Gjerësia","mm","884"]
["","","","Thellësia","mm","388"]
["Pesha","Njësia","","","kg","58.5"]
["Diapazoni i funksionimit","Ftohja","","Min.","°CDB","10"]
["","","","Maks.","°CDB","43"]
["","Ujë i ngrohtë në shtëpi","","Min.","°CDB","-25"]
["","Ujë i ngrohtë për përdorim në shtëpi","","Maks.","°CDB","35"]
["Niveli i fuqisë së zhurmës","Ngrohje","","Nom.","dBA","60 (1)"]
["","Ftohje","","Nom.","dBA","62 (1)"]
["Niveli i presionit të zhurmës","Ngrohje","","Nom.","dBA","47 (1)"]
["","Ftohje","","Nom.","dBA","49 (1)"]
["Agjenti ftohës","Lloji","","","","R-32"]
["","GWP","","","","675.0"]
["","Mbushja","","","tCO2Eq","1.01"]
["","Mbushja","","","kg","1.50"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","6"]
["","Gazi","","Dia. jasht.","mm","15.9"]
["","Kullimi","","Diametri i jashtëm","mm","18"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","30.0"]
["","Termoizolimi","","","","Tuba lëngu dhe gazi"]
["Furnizimi me energji","Emri","","","","V3"]
["","Faza","","","","1N~"]
["","Frekuenca","","","Hz","50"]
["","Tensioni","","","V","230"]
["Aktuale","Siguresat e rekomanduara","","","A","20"]
["Shënime","","","","","(1) - Ftohja Ta 35°C - LWE 18°C (DT = 5°C); Ngrohja Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]