{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSH-D"]
[]
[]
[]
[]
["","","","","","ETSH16P30DA","ETSH16P50DA"]
["Niveli i presionit të zhurmës","Nom.","","","dBA","32.8","32.8"]
["Diapazoni i funksionimit","Ftohja","Ambienti","Min.","°CDB","10","10"]
["","","Ana e ujit","Maks.","°C","22","22"]
["","","","Min.","°C","5","5"]
["","Ngrohje","Ana e ujit","Maks.","°C","70","70"]
["","","","Min.","°C","15","15"]
["Niveli i fuqisë së zhurmës","Nom.","","","dBA","45.6","45.6"]
["Dimensionet","Njësia","","Gjerësia","mm","590","785"]
["","","","Thellësia","mm","615","785"]
["","","","Lartësia","mm","1,891","1,896"]
["Veshja e jashtme","Material","","","","Polipropilen rezistent ndaj goditjeve","Polipropilen rezistent ndaj goditjeve"]
["","Ngjyra","","","","E bardhë trafiku (RAL9016) / Gri e errët (RAL7011)","E bardhë trafiku (RAL9016) / Gri e errët (RAL7011)"]
["PED","Category","","","","Art. 4.3","Art. 4.3"]
["Pesha","Njësia","","","kg","73","90"]
["Power supply","Faza","","","","1~","1~"]
["","Frekuenca","","","Hz","50","50"]
["","Tensioni","","","V","230","230"]
["Ngrohësi elektrik","Furnizimi me energji","","Frekuenca","Hz","50","50"]
["","","","Emri","","3V / 9W","3V / 9W"]
["","","","Faza","","1~ / 3~","1~ / 3~"]
["Shënime","","","","","(1) - Humbja e nxehtësisë sipas EN12897","(1) - Humbja e nxehtësisë sipas EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃"]