{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":11,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSX12E / EPRA08-12EV"]
[]
[]
[]
[]
["","","","","","ETSX12P30EF / EPRA08EAV3","ETSX12P50EF / EPRA08EAV3","ETSX12P30EF / EPRA10EAV3","ETSX12P50EF / EPRA10EAV3","ETSX12P30EF / EPRA12EAV3","ETSX12P50EF / EPRA12EAV3"]
["Indoor unit","","","","","ETSX12P30EF","ETSX12P50EF","ETSX12P30EF","ETSX12P50EF","ETSX12P30EF","ETSX12P50EF"]
["Kapaciteti ngrohës","Nom.","","","kW","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)"]
["Kapaciteti ftohës","Nom.","","","kW","6.81 (2)","6.81 (2)","7.97 (2)","7.97 (2)","8.62 (2)","8.62 (2)"]
["Fuqia në hyrje","Ngrohje","","Nom.","kW","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)"]
["","Ftohje","","Nom.","kW","2.15 (2)","2.15 (2)","2.66 (2)","2.66 (2)","2.96 (2)","2.96 (2)"]
["COP","","","","","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)"]
["EER","","","","","3.17 (2)","3.17 (2)","3","3","2.91 (2)","2.91 (2)"]
["Ngrohje uji të ngrohtë shtëpiak","Të përgjithshme","","Profili i deklaruar i ngarkesës","","L","XL","L","XL","L","XL"]
["","Klimë mesatare","","Kategoria e efikasitetit të energjisë të ngrohjes së ujit","","A+","A+","A+","A+","A+","A+"]
["Ngrohja e ambientit","Dalja e ujit për klimë mesatare 55°C","Të përgjithshme","SCOP","","3.47","3.47","3.48","3.48","3.48","3.48"]
["","Dalja e ujit klimë mesatare 55°C","Të përgjithshme","Klas. efikasitetit të ngrohjes sezonale të ambientit","","A++","A++","A++","A++","A++","A++"]
["","Dalja e ujit për klimë mesatare 35°C","Të përgjithshme","SCOP","","4.79","4.79","4.82","4.82","4.82","4.82"]
["","Dalja e ujit klimë mesatare 35°C","Të përgjithshme","Klas. efikasitetit të ngrohjes sezonale të ambientit","","A+++","A+++","A+++","A+++","A+++","A+++"]
["Shënime","","","","","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Kushti 1: ftohje Ta 35°C - LWE 18℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Kushti 2: ftohje Ta 35°C - LWE 7℃ (DT = 5°C); ngrohje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]
["","","","","","(3) - Kushti: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Kushti: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Kushti: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Kushti: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Kushti: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Kushti: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(4) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) me pompë në shpejtësi të plotë","(4) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) me pompë në shpejtësi të plotë","(4) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) me pompë në shpejtësi të plotë","(4) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) me pompë në shpejtësi të plotë","(4) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) me pompë në shpejtësi të plotë","(4) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) me pompë në shpejtësi të plotë"]