{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Veshja e jashtme","Ngjyra","","","","E bardhë","E bardhë"]
["","Materiali","","","","Rrëshirë","Rrëshirë"]
["Dimensionet","Njësia","","Lartësia","mm","290","340"]
["","","","Gjerësia","mm","1050","1200"]
["","","","Thellësia","mm","269","262"]
["Pesha","Njësia","","","kg","14","18"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","16.2","23"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","13.4","21.1"]
["","","","I ulët","m³/min","12.1","18.7"]
["","","Ngrohje","I lartë","m³/min","16.9","23"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","14.2","20.9"]
["","","Ngrohje","I ulët","m³/min","12.7","18.7"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","61","65"]
["","Ngrohje","","","dBA","61","65"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","45","49"]
["","","","Mesatar","dBA","42","45"]
["","","","I ulët","dBA","40","41"]
["","Ngrohje","","I lartë","dBA","45","49"]
["","","","Mesatar","dBA","42","45"]
["","","","I ulët","dBA","40","41"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","9.52","9.52"]
["","Gazi","","Dia. jasht.","mm","15.9","15.9"]
["","Kullimi","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Furnizimi me energji","Faza","","","","1~","1~"]
["","Frekuenca","","","Hz","50","50"]
["","Tensioni","","","V","220-240","220-240"]
["Aksesore Standarde","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Shënime","","","","","(1) - Kapacitetet nominale të ftohjes bazohen në: temperatura e brendshme: 27°CDB, 19°CWB, temp. e jashtme: 35°CDB, tubacioni i barasvlershëm i agjentit ftohës: 5m, diferenca e nivelit: 0m."]
["","","","","","(2) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m."]
["Aksesore Standarde","Screw cover","","","","","3"]