{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9"]
[]
[]
[]
[]
["","","","","FAQ71CVEB9","FAQ100CVEB9"]
["Niveli i presionit të zhurmës","Ngrohje","I lartë","dBA","45","49"]
["","","Nom.","dBA","42","45"]
["","","Mesatar","dBA","42","45"]
["","","I ulët","dBA","40","41"]
["","Ftohje","Mesatar","dBA","42","45"]
["","","I ulët","dBA","40","41"]
["","","I lartë","dBA","45","49"]
["","","Nom.","dBA","42","45"]
["Kapaciteti ftohës","Kapaciteti total","Nom.","kW","0.051","0.061"]
["Lidhjet e tubacioneve","Lëngu","Dia. jasht.","mm","9.52","9.52"]
["","Gazi","Dia. jasht.","mm","15.9","15.9"]
["","Kullimi","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Niveli i fuqisë së zhurmës","Ftohje","","dBA","61","65"]
["","Ngrohje","","dBA","61","65"]
["Dimensionet","Njësia","Gjerësia","mm","1,050","1,200"]
["","","Thellësia","mm","238","240"]
["","","Lartësia","mm","290","340"]
["Veshja e jashtme","Materiali","","","Rrëshirë","Rrëshirë"]
["","Colour","","","E bardhë e freskët","E bardhë e freskët"]
["Pesha","Njësia","","kg","13","17"]
["Kapaciteti ngrohës","Kapaciteti total","Nom.","kW","0.068","0.061"]
["Power supply","Phase","","","1~","1~"]
["","Frekuenca","","Hz","50","50"]
["","Tensioni","","V","220-240","220-240"]