{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZQSG100L8Y1B","FBA50A2VEB / FBA50A2VEB / RZQSG100L8Y1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZQSG125L8Y1B","FBA50A2VEB / FBA50A2VEB / FBA50A2VEB / RZQSG125L8Y1B","FBA60A2VEB / FBA60A2VEB / RZQSG125L8Y1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZQSG140L7Y1B"]
["Kapaciteti ftohës","Nom.","","kW","9.50 (1)","9.50 (1)","12.0 (1)","","12.0 (1)","13.4 (1)"]
["Space cooling","SEER","","","5.10","5.10","4.80","4.80","4.80"]
["","Konsumi vjetor i energjisë","","kWh/a","652","652","875","875","875"]
["","Kapaciteti","Pdesign","kW","9.50","9.50","12.0","12.0","12.0"]
["","Kategoria e efikasitetit të energjisë","","","A","A","B","B","B"]
["Ngrohja e hapësirës (klimë mesatare)","Kapaciteti","Pdesign","kW","7.60","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","3.80","3.80","3.80","3.80","3.80"]
["","Kategoria e efikasitetit të energjisë","","","A","A","A","A","A"]
["","Konsumi vjetor i energjisë","","kWh/a","2,800","2,800","2,800","2,800","2,800"]
["Efikasiteti nominal","EER","","","3.28 (3)","3.06 (3)","3.04 (3)","","2.83 (3)","4.20 (3)"]
["","COP","","","3.33 (3)","3.30 (3)","3.35 (3)","","3.26 (3)"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A","B","B","","C"]
["","","Ngrohje","","C","C","C","","C"]
["Kapaciteti ngrohës","Nom.","","kW","10.8 (2)","10.8 (2)","13.5 (2)","","13.5 (2)","15.5 (2)"]
["Shënime","","","","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m"]
["","","","","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m"]
["","","","","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së"]