{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":6,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RXS-K"]
[]
[]
[]
[]
["","","","","FBQ35C8VEB / RXS35K2V1B","FBQ50C8VEB / RXS50K2V1B"]
["Kapaciteti ftohës","Nom.","","kW","3.40","5.00"]
["Efikasiteti nominal","Annual energy consumption","","kWh","530","825"]
["","EER","","","3.21","3.03"]
["","COP","","","3.51","3.42"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A","B"]
["","","Ngrohje","","B","B"]
["Kapaciteti i ngrohjes","Nom.","","kW","4.00","5.50"]
["Shënime","","","","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së"]
["","","","","(2) - Efikasiteti nominal: ftohje në ngarkesë nominale 35°/27°, ngrohje në ngarkesë nominale 7°/20°","(2) - Efikasiteti nominal: ftohje në ngarkesë nominale 35°/27°, ngrohje në ngarkesë nominale 7°/20°"]