{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / AZQS-BY1"]
[]
[]
[]
[]
["","","","","FCAG100AVEB / AZQS100B7Y1B","FCAG125AVEB / AZQS125B7Y1B","FCAG140AVEB / AZQS140B7Y1B"]
["Kapaciteti ftohës","Nom.","","kW","9.50 (1)","12.1 (1)","13.0 (1)"]
["Ftohja e hapësirës","SEER","","","5.50","5.16","5.94"]
["","Konsumi vjetor i energjisë","","kWh/a","605","1,406","1,314"]
["","Kapaciteti","Pdesign","kW","9.50","12.1","13.0"]
["","Kategoria e efikasitetit të energjisë","","","A"]
["Ngrohja e hapësirës (klimë mesatare)","Kapaciteti","Pdesign","kW","7.60","7.78","11.6"]
["","SCOP/A","","","3.85","3.67","3.96"]
["","Kategoria e efikasitetit të energjisë","","","A"]
["","Konsumi vjetor i energjisë","","kWh/a","2,764","2,969","4,089"]
["Efikasiteti nominal","Annual energy consumption","","kWh","1,480"]
["","EER","","","3.21 (3)","2.22 (3)","2.63 (3)"]
["","COP","","","3.50 (3)","3.41 (3)","3.30 (3)"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A"]
["","","Ngrohje","","B"]
["Kapaciteti ngrohës","Nom.","","kW","10.8 (2)","13.5 (2)","15.5 (2)"]
["Shënime","","","","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m"]
["","","","","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m"]
["","","","","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së"]