{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":24,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FCAG100AVEB / RZQG71L9V1B","FCAG100AVEB / RZQG100L9V1B","FCAG50AVEB / FCAG50AVEB / FCAG50AVEB / RZQG125L9V1B","FCAG60AVEB / FCAG60AVEB / RZQG125L9V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG100L9V1B","FCAG50AVEB / FCAG50AVEB / RZQG100L9V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG125L9V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG71L9V1B","FCAG35AVEB / FCAG35AVEB / RZQG71L9V1B","FCAG50AVEB / FCAG50AVEB / RZQG71L9V1B","FCAG71AVEB / RZQG71L9V1B","FCAG140AVEB / RZQG100L9V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG100L9V1B","FCAG50AVEB / FCAG50AVEB / FCAG50AVEB / RZQG100L9V1B","FCAG71AVEB / FCAG71AVEB / RZQG100L9V1B","FCAG125AVEB / RZQG125L9V1B","FCAG140AVEB / RZQG125L9V1B","FCAG71AVEB / FCAG71AVEB / RZQG125L9V1B","FCAG140AVEB / RZQG140L9V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG140L9V1B"]
["Gama e efikasitetit të energjisë","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Ftohja e hapësirës","SEER","","","","","","","","","","5.10","5.10","5.10","6.72","6.80","","","","6.00","6.00","5.10","6.44","9.70"]
["","Konsumi vjetor i energjisë","","kWh/a","","","","","","","","467","467","467","355","489","","","","700","700","824","1,249","829"]
["","Kapaciteti","Pdesign","kW","","","","","","","","6.80","6.80","6.80","6.80","9.50","","","","12.0","12.00","12.0","13.4","13.4"]
["","Kategoria e efikasitetit të energjisë","","","","","","","","","","A","A","A","A++","A++","","","","A+","A+","A"]
["Ngrohja e hapësirës (klimë mesatare)","Kapaciteti","Pdesign","kW","","","","","","","","6.00","6.00","6.00","6.33","11.30","","","","12.7","12.66","12.7","11.6","12.0"]
["","SCOP/A","","","","","","","","","","3.80","3.80","3.80","4.20","4.61","","","","4.10","4.10","3.80","4.27","3.96"]
["","Kategoria e efikasitetit të energjisë","","","","","","","","","","A","A","A","A+","A++","","","","A+","A+","A"]
["","Konsumi vjetor i energjisë","","kWh/a","","","","","","","","2,211","2,211","2,211","2,110","3,432","","","","4,323","4,323","4,683","3,795","4,235"]
["Shënime","","","","","","","","","","","","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","","","","","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","","","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m"]
["","","","","","","","","","","","","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m","","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m","","","","","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m","","","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m"]
["","","","","","","","","","","","","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","","","","","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","","","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së"]
["Kapaciteti ftohës","Nom.","","kW","","","","","","","","","","","6.80 (1)","","","","","12.0 (1)","","","13.4 (1)","13.4 (1)"]
["Efikasiteti nominal","Annual energy consumption","","kWh","","","","","","","","","","","1,005","","","","","1,610"]
["","EER","","","","","","","","","","","","","3.39 (3)","","","","","3.73 (3)","","","2.50 (3)","4.29 (3)"]
["","COP","","","","","","","","","","","","","3.97 (3)","","","","","3.63 (3)","","","3.61 (3)"]
["","Direktiva e etiketimit të energjisë","Ftohje","","","","","","","","","","","","A","","","","","A"]
["","","Ngrohje","","","","","","","","","","","","A","","","","","A"]
["Kapaciteti i ngrohjes","Nom.","","kW","","","","","","","","","","","7.50 (2)","","","","","13.5 (2)","","","15.5 (2)","15.5 (2)"]
["Outdoor unit","","","","","","","","","","","","","","","","RZQG100L9V1","RZQG100L9V1","RZQG100L9V1"]
["Ftohja e hapësirës","Kategoria e efikasitetit të energjisë","","","","","","","","","","","","","","","A","A","A"]
["","Kapaciteti","Pdesign","kW","","","","","","","","","","","","","9.50","9.50","9.50"]
["","SEER","","","","","","","","","","","","","","","5.10","5.10","5.10"]
["","Konsumi vjetor i energjisë","","kWh/a","","","","","","","","","","","","","652","652","652"]
["Ngrohja e hapësirës (klimë mesatare)","Kategoria e efikasitetit të energjisë","","","","","","","","","","","","","","","A","A","A"]
["","Kapaciteti","Pdesign","kW","","","","","","","","","","","","","7.60","11.3","11.3"]
["","SCOP/A","","","","","","","","","","","","","","","3.80","3.80","3.80"]
["","Pdh Kapaciteti i ngrohjes në -10°","","kW","","","","","","","","","","","","","6.95"]
["","Konsumi vjetor i energjisë","","kWh/a","","","","","","","","","","","","","4164","4164","4164"]
["Ftohja e hapësirës","ηs,c","","%","","","","","","","","","","","","","","","","","","","254.6","385.1"]
["Ngrohja e hapësirës (klimë mesatare)","ηs,h","","%","","","","","","","","","","","","","","","","","","","167.6","155.2"]