{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":15,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FCAG50AVEB / FCAG50AVEB / FCAG50AVEB / RZQSG125L9V1B","FCAG60AVEB / FCAG60AVEB / RZQSG125L9V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQSG125L9V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQSG100L9V1B","FCAG50AVEB / FCAG50AVEB / RZQSG100L9V1B","FCAG71AVEB / RZQSG71L3V1B","FCAG35AVEB / FCAG35AVEB / RZQSG71L3V1B","FCAG100AVEB / RZQSG100L9V1B","FCAG125AVEB / RZQSG125L9V1B","FCAG140AVEB / RZQSG140L9V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQSG140L9V1B"]
["Kapaciteti ftohës","Nom.","","kW","","","","","","6.80 (1)","","9.50 (1)","12.0 (1)","13.4 (1)","13.4 (1)"]
["Ftohja e hapësirës","SEER","","","","","","","","6.10","5.10","6.50","5.30"]
["","Konsumi vjetor i energjisë","","kWh/a","","","","","","391","467","512","793"]
["","Kapaciteti","Pdesign","kW","","","","","","6.80","6.80","9.50","12.0"]
["","Kategoria e efikasitetit të energjisë","","","","","","","","A++","A","A++","A"]
["Ngrohja e hapësirës (klimë mesatare)","Kapaciteti","Pdesign","kW","","","","","","6.33","6.00","7.60","8.03"]
["","SCOP/A","","","","","","","","4.10","3.80","4.10","4.01"]
["","Kategoria e efikasitetit të energjisë","","","","","","","","A+","A","A+","A+"]
["","Konsumi vjetor i energjisë","","kWh/a","","","","","","2,162","2,211","2,596","2,804"]
["Efikasiteti nominal","Annual energy consumption","","kWh","","","","","","1,060","","1,440","1,870"]
["","EER","","","","","","","","3.21 (3)","","3.30 (3)","3.21 (3)","2.40 (3)","4.20 (3)"]
["","COP","","","","","","","","3.61 (3)","","3.54 (3)","3.41 (3)","3.41 (3)"]
["","Direktiva e etiketimit të energjisë","Ftohje","","","","","","","A","","A","A"]
["","","Ngrohje","","","","","","","A","","B","B"]
["Kapaciteti ngrohës","Nom.","","kW","","","","","","7.50 (2)","","10.8 (2)","13.5 (2)","15.5 (2)","15.5 (2)"]
["Shënime","","","","","","","","","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m"]
["","","","","","","","","","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m"]
["","","","","","","","","","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së"]
["Gama e efikasitetit të energjisë","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]