{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":13,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100GVEB / RZQG100L8Y1B","FCAHG125GVEB / RZQG125L8Y1B","FCAHG100GVEB / RZQG71L8Y1B","FCAHG71GVEB / RZQG71L8Y1B","FCAHG140GVEB / RZQG100L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG100L8Y1B","FCAHG140GVEB / RZQG125L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG140L7Y1B"]
["Kapaciteti ftohës","Nom.","","kW","","","","6.80 (1)","","","","","13.4 (1)"]
["Ftohja e hapësirës","SEER","","","","","6.91","6.91","","","","","6.75"]
["","ηs,c","","%","","","","","","","","","266.9"]
["","Konsumi vjetor i energjisë","","kWh/a","","","345","345","","","","","1,191"]
["","Kapaciteti","Pdesign","kW","","","6.80","6.80","","","","","13.4"]
["","Kategoria e efikasitetit të energjisë","","","","","A++","A++"]
["Ngrohja e hapësirës (klimë mesatare)","Kapaciteti","Pdesign","kW","","","7.60","7.60","","","","","11.8"]
["","SCOP/A","","","","","4.54","4.54","","","","","4.38"]
["","Kategoria e efikasitetit të energjisë","","","","","A+","A+"]
["","Konsumi vjetor i energjisë","","kWh/a","","","2,344","2,344","","","","","3,766"]
["","ηs,h","","%","","","","","","","","","172.1"]
["Efikasiteti nominal","Konsumi vjetor i energjisë","","kWh","","","","830"]
["","EER","","","","","","4.09 (3)","","","","","3.18 (3)"]
["","COP","","","","","","4.80 (3)","","","","","4.12 (3)"]
["","Direktiva e etiketimit të energjisë","Ftohje","","","","","A"]
["","","Ngrohje","","","","","A"]
["Kapaciteti ngrohës","Nom.","","kW","","","","7.50 (2)","","","","","15.5 (2)"]
["Gama e efikasitetit të energjisë","","","","A+++ ~ D","A+++ ~ D","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Shënime","","","","","","","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","","","","","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m"]
["","","","","","","","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m","","","","","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m"]
["","","","","","","","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","","","","","(3) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së"]
["Njësia e jashtme","","","","","","","","","RZQG100L8Y1","","RZQG125L8Y1"]
["Ftohja e hapësirës","Kategoria e efikasitetit të energjisë","","","","","","","","A","","A"]
["","Kapaciteti","Pdesign","kW","","","","","","9.50","","12.0"]
["","SEER","","","","","","","","5.10","","5.10"]
["","Konsumi vjetor i energjisë","","kWh/a","","","","","","652","","824"]
["Ngrohja e hapësirës (klimë mesatare)","Kategoria e efikasitetit të energjisë","","","","","","","","A","","A"]
["","Kapaciteti","Pdesign","kW","","","","","","11.30","","12.71"]
["","SCOP/A","","","","","","","","3.80","","3.80"]
["","Pdh Kapaciteti i ngrohjes në -10°","","kW","","","","","","9.66","","11.4"]
["","Konsumi vjetor i energjisë","","kWh/a","","","","","","4164","","4683"]