{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":14,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCQG71FVEB / RZQG71L8Y1B","FCQG100FVEB / RZQG71L8Y1B","FCQG35FVEB / FCQG35FVEB / RZQG71L8Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG100L8Y1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQG100L8Y1B","FCQG140FVEB / RZQG100L8Y1B","FCQG71FVEB / FCQG71FVEB / RZQG100L8Y1B","FCQG140FVEB / RZQG125L8Y1B","FCQG71FVEB / FCQG71FVEB / RZQG125L8Y1B","FCQG140FVEB / RZQG140L7Y1B"]
["Kapaciteti ftohës","Nom.","","kW","6.8","","","","","","","","","13.4"]
["Ftohja e hapësirës","SEER","","","6.72","6.80","5.1","5.10","5.10","6.80","5.10","6.00","5.10"]
["","Konsumi vjetor i energjisë","","kWh/a","355","350","467","652","652","489","652","700","824"]
["","Kapaciteti","Pdesign","kW","6.80","6.80","6.8","9.50","9.50","9.50","9.50","12.00","12.00"]
["","Kategoria e efikasitetit të energjisë","","","A++","A++","B","B","B","A++","B","A+","B"]
["Ngrohja e hapësirës (klimë mesatare)","Kapaciteti","Pdesign","kW","6.33","6.33","6","11.30","11.30","11.30","11.30","12.66","12.71"]
["","SCOP/A","","","4.20","4.20","3.8","3.80","3.80","4.61","3.80","4.10","3.80"]
["","Kategoria e efikasitetit të energjisë","","","A+","A+","A","A","A","A++","A","A+","A"]
["","Konsumi vjetor i energjisë","","kWh/a","2,110","2,110","2,211","4,164","4,164","3,432","4,164","4,323","4,683"]
["Efikasiteti nominal","Annual energy consumption","","kWh","1,005"]
["","EER","","","3.39","","","","","","","","","3.21"]
["","COP","","","3.97","","","","","","","","","3.61"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A"]
["","","Ngrohje","","A"]
["Kapaciteti ngrohës","Nom.","","kW","7.5","","","","","","","","","15.5"]
["Shënime","","","","(1) - Konsumi vjetor i energjisë është në përputhje me Direktivën e etiketimit të energjisë 2002/31/EC","","","","","","","","","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së"]
["","","","","(2) - SEER dhe SCOP janë në përputhje me EN 14825","","","","","","","","","(2) - Efikasiteti nominal: ftohje në ngarkesë nominale 35°/27°, ngrohje në ngarkesë nominale 7°/20°"]
["","","","","","","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së"]