{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":12,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCQG50FVEB / FCQG50FVEB / RZQSG100L8Y1B","FCQG100FVEB / RZQSG100L8Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG100L8Y1B","FCQG125FVEB / RZQSG125L8Y1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQSG125L8Y1B","FCQG60FVEB / FCQG60FVEB / RZQSG125L8Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG125L8Y1B","FCQG140FVEB / RZQSG140L7Y1B"]
["Kapaciteti ftohës","Nom.","","kW","","9.5","","12.0","","","","13.4"]
["Ftohja e hapësirës","SEER","","","5.1","6.5","5.1","5.3","4.8","4.8","4.8"]
["","Konsumi vjetor i energjisë","","kWh/a","652","512","652","793","875","875","875"]
["","Kapaciteti","Pdesign","kW","9.5","9.5","9.5","12","12","12","12"]
["","Kategoria e efikasitetit të energjisë","","","B","A++","B","A","B","B","B"]
["Ngrohja e hapësirës (klimë mesatare)","Kapaciteti","Pdesign","kW","7.6","7.6","7.6","8.03","7.6","7.6","7.6"]
["","SCOP/A","","","3.8","4.1","3.8","4.01","3.8","3.8","3.8"]
["","Kategoria e efikasitetit të energjisë","","","A","A+","A","A+","A","A","A"]
["","Konsumi vjetor i energjisë","","kWh/a","2,800","2,596","2,800","2,804","2,800","2,800","2,800"]
["Efikasiteti nominal","Konsumi vjetor i energjisë","","kWh","","1,440","","1,870","","","","2,225"]
["","EER","","","","3.30","","3.21","","","","3.01"]
["","COP","","","","3.54","","3.41","","","","3.41"]
["","Direktiva e etiketimit të energjisë","Ftohje","","","A","","A"]
["","","Ngrohje","","","A","","B"]
["Kapaciteti ngrohës","Nom.","","kW","","10.8","","13.5","","","","15.5"]
["Shënime","","","","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së"]
["","","","","","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","","","","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së"]
["","","","","","(2) - Efikasiteti nominal: ftohje në ngarkesë nominale 35°/27°, ngrohje në ngarkesë nominale 7°/20°","","(2) - Efikasiteti nominal: ftohje në ngarkesë nominale 35°/27°, ngrohje në ngarkesë nominale 7°/20°","","","","(2) - Efikasiteti nominal: ftohje në ngarkesë nominale 35°/27°, ngrohje në ngarkesë nominale 7°/20°"]
["","","","","","(3) - Konsumi vjetor i energjisë është në përputhje me Direktivën e etiketimit të energjisë 2002/31/EC","","(3) - Konsumi vjetor i energjisë është në përputhje me Direktivën e etiketimit të energjisë 2002/31/EC"]
["","","","","","(4) - SEER dhe SCOP janë në përputhje me EN 14825","","(4) - SEER dhe SCOP janë në përputhje me EN 14825"]