{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDBQ-B"]
[]
[]
[]
[]
["","","","","","FDBQ25B5V1","FDBQ25B8V1"]
["Niveli i presionit të zhurmës","Ngrohje","","I lartë","dBA","35.0","35.0"]
["","","","I ulët","dBA","29.0","29.0"]
["","Ftohje","","I ulët","dBA","28.0","28.0"]
["","","","I lartë","dBA","35.0","35.0"]
["Aksesore Standarde","Manual instalimi dhe përdorimi","","","","1","1"]
["","Filtër për thithjen e ajrit","","","","1","1"]
["Sisteme kontrolli","Wired remote control","","","","BRC1D52, BRC1E52A/B"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","6.35"]
["","Gazi","","Dia. jasht.","mm","9.52"]
["","Kullimi","","","","27.2"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","55","55"]
["","Ngrohje","","","dBA","55","55"]
["Dimensionet","Njësia","","Gjerësia","mm","652","652"]
["","","","Thellësia","mm","502","502"]
["","","","Lartësia","mm","230","230"]
["Veshja e jashtme","Materiali","","","","Çelik me pak karbon, i veshur me zink","Çelik me pak karbon, i veshur me zink"]
["Pesha","Njësia","","","kg","17.0","17.0"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ngrohje","I lartë","m³/min","","6.95"]
["","","","I ulët","m³/min","","5.20"]
["","","Ftohje","I ulët","m³/min","","5.20"]
["","","","I lartë","m³/min","","6.50"]
["Power supply","Phase","","","","1~","1~"]
["","Frekuenca","","","Hz","50","50"]
["","Emri","","","","V1","V1"]
["","Tensioni","","","V","230","230 +/-10%"]
["Shënime","","","","","(1) - Vlerat e zhurmës janë matur në një dhomë gjysëm anakoike.","(1) - Vlerat e zhurmës janë matur në një dhomë gjysëm anakoike."]
["","","","","","(2) - Niveli i presionit të zhurmës është vlerë relative në varësi të distancës dhe ambientit akustik. Për më shumë detaje, ju lutem referojuni skicave të nivelit të zhurmës.","(2) - Niveli i presionit të zhurmës është vlerë relative në varësi të distancës dhe ambientit akustik. Për më shumë detaje, ju lutem referojuni skicave të nivelit të zhurmës."]
["","","","","","(3) - Niveli i fuqisë së zhurmës është vlerë absolute dhe tregon fuqinë që prodhon një burim zhurme.","(3) - Niveli i fuqisë së zhurmës është vlerë absolute dhe tregon fuqinë që prodhon një burim zhurme."]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","","6.35"]
["","Gazi","","Dia. jasht.","mm","","9.52"]
["","Kullimi","","","","","27.2"]