{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F"]
[]
[]
[]
[]
["","","","","FDXM25F2V1B","FDXM35F2V1B","FDXM50F2V1B","FDXM60F2V1B"]
["Niveli i presionit të zhurmës","Ngrohje","I lartë","dBA","35","35","38","38"]
["","","I ulët","dBA","27","27","30","30"]
["","Ftohje","I ulët","dBA","27","27","30","30"]
["","","I lartë","dBA","35","35","38","38"]
["","","Nom.","dBA","33","33","36","36"]
["","Ftohje","Nom.","dBA","33","33","36","35"]
["Sisteme kontrolli","Wired remote control","","","BRC1D52, BRC1E51A","BRC1D52, BRC1E51A","BRC1D52, BRC1E51A","BRC1D52, BRC1E51A"]
["","Infrared remote control","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Lidhjet e tubacioneve","Lëngu","Dia. jasht.","mm","6.35","6.35","6.35","6.35"]
["","Gazi","Dia. jasht.","mm","9.5","9.5","12.7","12.7"]
["","Kullimi","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Fuqia në hyrje","Ftohje","Nom.","kW","0.036","0.036","0.060","0.060"]
["","Ngrohje","Nom.","kW","0.036","0.036","0.060","0.060"]
["Niveli i fuqisë së zhurmës","Ftohje","","dBA","53","53","55","56"]
["","Ngrohje","","dBA","53","53","55","56"]
["Dimensionet","Njësia","Gjerësia","mm","750","750","1,150","1,150"]
["","","Thellësia","mm","620","620","620","620"]
["","","Lartësia","mm","200","200","200","200"]
["Pesha","Njësia","","kg","21","21","30","30"]
["Ventilatori","Presioni i jashtëm statik","Nom.","Pa","30","30","40","40"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Frekuenca","","Hz","50","50","50","50"]
["","Emri","","","V1","V1","V1","V1"]
["","Tensioni","","V","230","230","220-240","220-240"]