{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Niveli i presionit të zhurmës","Ngrohje","","I lartë","dBA","35.0","35.0","","38.0"]
["","","","Mesatar","dBA","33.0","33.0","","35.0"]
["","","","I ulët","dBA","27.0","27.0","","30.0"]
["","Ftohje","","Mesatar","dBA","33.0","33.0","","35.0"]
["","","","I ulët","dBA","27.0","27.0","","30.0"]
["","","","I lartë","dBA","35.0","35.0","","38.0"]
["Aksesore Standarde","Manual instalimi","","","","1","1","","1"]
["","Manual përdorimi","","","","1","1","","1"]
["","Izolues për rakorderi","","","","1","1","","1"]
["","Tampon izolues","","","","1","1","","1"]
["","Metal mbërthimi","","","","1","1","","1"]
["","Zorrë kullimi","","","","1","1","","1"]
["","Rondele për varëset","","","","8","8","","8"]
["","Material izolues","","","","2","2","","2"]
["","Mbërthyes","","","","6","6","","6"]
["","Pllakë fiksimi për rondelën","","","","4","4","","4"]
["","Vida për flanxhat e tubave","","","","1","1","","1"]
["","Filtër ajri","","","","1","1","","1"]
["Lidhjet e tubacioneve","Liquid","","OD","mm","6.35","6.35","","6.35"]
["","Gazi","","Diametri i jashtëm","mm","9.50","9.50","","12.70"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Power input","Ftohje","","Nom.","kW","0.036","0.036","","0.060"]
["","Ngrohje","","Nom.","kW","0.036","0.036","","0.060"]
["Sound power level","Ftohje","","","dBA","53.0","53.0","","56.0"]
["","Ngrohje","","","dBA","53.0","53.0","","56.0"]
["Dimensionet","Njësia","","Gjerësia","mm","750","750","","1,150"]
["","","","Thellësia","mm","620","620","","620"]
["","","","Lartësia","mm","200","200","","200"]
["Pesha","Njësia","","","kg","21","21","","28"]
["Ventilatori","Presioni i jashtëm statik","","Nom.","Pa","30","30","","40"]
["","Niveli i qarkullimit të ajrit","Ngrohje","I lartë","m³/min","8.7","8.7","","16.0"]
["","","","Mesatar","m³/min","8.0","8.0","","14.8"]
["","","","I ulët","m³/min","7.3","7.3","","13.5"]
["","","Ftohje","I ulët","m³/min","7.3","7.3","","13.5"]
["","","","Mesatar","m³/min","8.0","8.0","","14.8"]
["","","","I lartë","m³/min","8.7","8.7","","16.0"]
["Power supply","Faza","","","","1~","1~","","1~"]
["","Frekuenca","","","Hz","50","50","","50"]
["","Tensioni","","","V","220-240","220-240","","220-240"]
["Shënime","","","","","(1) - Shiko skicën e veçantë për të dhënat e skicave elektrike","(1) - Shiko skicën e veçantë për të dhënat e skicave elektrike","","(1) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","","","0.060"]
["","Ngrohje","","Nom.","kW","","","0.060"]
["Dimensionet","Njësia","","Lartësia","mm","","","200"]
["","","","Gjerësia","mm","","","1150"]
["","","","Thellësia","mm","","","620"]
["Pesha","Njësia","","","kg","","","28"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","","","15.8"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","","","14.6"]
["","","","I ulët","m³/min","","","13.3"]
["","","Ngrohje","I lartë","m³/min","","","15.8"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","","","14.6"]
["","","Ngrohje","I ulët","m³/min","","","13.3"]
["","Presioni i jashtëm statik","","Nom.","Pa","","","40"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","","","55.0"]
["","Ngrohje","","","dBA","","","55.0"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","","","38.0"]
["","","","Mesatar","dBA","","","35.0"]
["","","","I ulët","dBA","","","30.0"]
["","Ngrohje","","I lartë","dBA","","","38.0"]
["","","","Mesatar","dBA","","","35.0"]
["","","","I ulët","dBA","","","30.0"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","","","6.35"]
["","Gazi","","Dia. jasht.","mm","","","12.70"]
["","Kullimi","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Aksesore Standarde","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Air filter","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Furnizimi me energji","Faza","","","","","","1~"]
["","Frekuenca","","","Hz","","","50"]
["","Tensioni","","","V","","","220-240"]