{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":10,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG100L8Y1B","FDXS60F2VEB / FDXS60F2VEB / RZQG125L8Y1B","FDXS35F2VEB / FDXS35F2VEB / RZQG71L8Y1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG71L8Y1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG100L8Y1B"]
["Ftohja e hapësirës","SEER","","","","","4.8","4.80","5.10"]
["","Konsumi vjetor i energjisë","","kWh/a","","","496","496","652"]
["","Kapaciteti","Pdesign","kW","","","6.8","6.80","9.50"]
["","Kategoria e efikasitetit të energjisë","","","","","B","B","B"]
["Ngrohja e hapësirës (klimë mesatare)","Kapaciteti","Pdesign","kW","","","6","6.00","10.74"]
["","SCOP/A","","","","","3.8","3.80","3.80"]
["","Kategoria e efikasitetit të energjisë","","","","","A","A","A"]
["","Konsumi vjetor i energjisë","","kWh/a","","","2,211","2,211","3,957"]
["Shënime","","","","","","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së"]
["Gama e efikasitetit të energjisë","","","","A+++ ~ D","A+++ ~ D","","","","A+++ ~ D"]