{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXM-N"]
[]
[]
[]
[]
["","","","","FFA50A2VEB / RXM50N2V1B","FFA60A2VEB / RXM60N2V1B"]
["Kapaciteti ftohës","Nom.","","kW","","5.70"]
["Kapaciteti ngrohës","Nom.","","kW","","7.00"]
["Efikasiteti nominal","EER","","","","3.05"]
["","COP","","","","3.41"]
["","Annual energy consumption","","kWh","","934"]
["","Direktiva e etiketimit të energjisë","Ftohje","","","B"]
["","","Ngrohje","","","B"]
["Ftohja e hapësirës","Kategoria e efikasitetit të energjisë","","","","A+"]
["","Kapaciteti","Pdesign","kW","","5.70"]
["","SEER","","","","5.76"]
["","Konsumi vjetor i energjisë","","kWh/a","","347"]
["Ngrohja e hapësirës (klimë mesatare)","Kategoria e efikasitetit të energjisë","","","","A+"]
["","Kapaciteti","Pdesign","kW","","3.96"]
["","SCOP/A","","","","4.04"]
["","Konsumi vjetor i energjisë","","kWh/a","","1,372"]
["Shënime","","","","","(1) - Shiko skicën e veçantë për diapazonin e funksionimit"]
["","","","","","(2) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]
["","","","","","(3) - Kapacitetet nominale të ftohjes bazohen në: temperatura e brendshme: 27°CDB, 19°CWB, temp. e jashtme: 35°CDB, tubacioni i barasvlershëm i agjentit ftohës: 5m, diferenca e nivelit: 0m."]
["","","","","","(4) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m."]
["Outdoor unit","","","","RXM50N2V1B"]
["Kapaciteti ftohës","Nom.","","kW","5.00"]
["Kapaciteti ngrohës","Nom.","","kW","5.80"]
["Efikasiteti nominal","EER","","","3.24"]
["","COP","","","3.49"]
["","Konsumi vjetor i energjisë","","kWh","771"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A"]
["","","Ngrohje","","B"]
["Ftohja e hapësirës","Kategoria e efikasitetit të energjisë","","","A+"]
["","Kapaciteti","Pdesign","kW","5.00"]
["","SEER","","","5.98"]
["","Konsumi vjetor i energjisë","","kWh/a","292"]
["Ngrohja e hapësirës (klimë mesatare)","Kategoria e efikasitetit të energjisë","","","A"]
["","Kapaciteti","Pdesign","kW","3.84"]
["","SCOP/A","","","3.90"]
["","Pdh Kapaciteti i ngrohjes në -10°","","kW","3.51"]
["","Konsumi vjetor i energjisë","","kWh/a","1377"]
["Gama e efikasitetit të energjisë","","","","A+++ ~ D"]