{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXM-N"]
[]
[]
[]
[]
["","","","","FFA50A2VEB / RXM50N2V1B","FFA60A2VEB / RXM60N2V1B"]
["Kapaciteti ftohës","Nom.","","kW","5.00","5.70"]
["Ftohja e hapësirës","Konsumi vjetor i energjisë","","kWh/a","","347"]
["","Kapaciteti","Pdesign","kW","","5.70"]
["Ngrohja e hapësirës (klimë mesatare)","Kapaciteti","Pdesign","kW","","3.96"]
["","Konsumi vjetor i energjisë","","kWh/a","","1,372"]
["Efikasiteti nominal","Annual energy consumption","","kWh","771","934"]
["","EER","","","3.24","3.05"]
["","COP","","","3.49","3.41"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A","B"]
["","","Ngrohje","","B","B"]
["Kapaciteti ngrohës","Nom.","","kW","5.80","7.00"]
["Shënime","","","","(1) - Shiko skicën e veçantë për diapazonin e funksionimit","(1) - Shiko skicën e veçantë për diapazonin e funksionimit"]
["","","","","(2) - Shiko skicën e veçantë për të dhënat e skicave elektrike","(2) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]
["","","","","(3) - Kapacitetet nominale të ftohjes bazohen në: temperatura e brendshme: 27°CDB, 19°CWB, temperatura e jashtme: 35°CDB, tubacioni i barasvlershëm i agjentit ftohës: 5m, diferenca e nivelit: 0m.","(3) - Kapacitetet nominale të ftohjes bazohen në: temperatura e brendshme: 27°CDB, 19°CWB, temp. e jashtme: 35°CDB, tubacioni i barasvlershëm i agjentit ftohës: 5m, diferenca e nivelit: 0m."]
["","","","","(4) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m.","(4) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m."]
["Ftohja e hapësirës","Kategoria e efikasitetit të energjisë","","","","A+"]
["","SEER","","","","5.76"]
["Ngrohja e hapësirës (klimë mesatare)","Kategoria e efikasitetit të energjisë","","","","A+"]
["","SCOP/A","","","","4.04"]