{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RXS-L3"]
[]
[]
[]
[]
["","","","","FHA35AVEB / RXS35L3V1B"]
["Njësia e jashtme","","","","RXS35L3V1B"]
["Kapaciteti ftohës","Nom.","","kW","3.40"]
["Kapaciteti ngrohës","Nom.","","kW","4.00"]
["Efikasiteti nominal","EER","","","3.70"]
["","COP","","","4.08"]
["","Konsumi vjetor i energjisë","","kWh","459"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A"]
["","","Ngrohje","","A"]
["Ftohja e hapësirës","Kategoria e efikasitetit të energjisë","","","A++"]
["","Kapaciteti","Pdesign","kW","3.40"]
["","SEER","","","6.18"]
["","Konsumi vjetor i energjisë","","kWh/a","193"]
["Ngrohja e hapësirës (klimë mesatare)","Kategoria e efikasitetit të energjisë","","","A+"]
["","Kapaciteti","Pdesign","kW","3.10"]
["","SCOP/A","","","4.43"]
["","Pdh Kapaciteti i ngrohjes në -10°","","kW","2.63"]
["","Konsumi vjetor i energjisë","","kWh/a","981"]