{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":6,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNQ-A / RXS-L"]
[]
[]
[]
[]
["","","","","FNQ50A2VEB / RXS50L2V1B","FNQ60A2VEB / RXS60L2V1B"]
["Kapaciteti i ftohjes","Nom.","","kW","5.0","6.0"]
["Efikasiteti nominal","Konsumi vjetor i energjisë","","kWh","746","1,119"]
["","EER","","","3.35 (1)","2.68 (1)"]
["","COP","","","3.34 (1)","3.11 (1)"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A","D"]
["","","Ngrohje","","C","D"]
["Kapaciteti i ngrohjes","Nom.","","kW","5.80","7.00"]
["Shënime","","","","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së"]
["","","","","(2) - Efikasiteti nominal: ftohje në ngarkesë nominale 35°/27°, ngrohje në ngarkesë nominale 7°/20°","(2) - Efikasiteti nominal: ftohje në ngarkesë nominale 35°/27°, ngrohje në ngarkesë nominale 7°/20°"]