{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":92,"n_cols":10,"rows_kept":92,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-AW"]
[]
[]
[]
[]
["","","","","","FTXA20A2V1BW","FTXA25A2V1BW","FTXA35A2V1BW","FTXA42A2V1BW","FTXA50A2V1BW"]
["Niveli i presionit të zhurmës","Ngrohje","","I lartë","dBA","39","40","41","","46"]
["","","","Mesatar","dBA","32","33","33","","42"]
["","","","Funksionim pa zhurmë","dBA","19","19","19","","24"]
["","","","I ulët","dBA","25","25","25","","33"]
["","Ftohje","","Mesatar","dBA","32","33","33","","39"]
["","","","Funksionim pa zhurmë","dBA","19","19","19","","24"]
["","","","I ulët","dBA","25","25","25","","31"]
["","","","I lartë","dBA","39","40","41","","46"]
["Aksesore Standarde","Manual instalimi","","","","1","1","1","","1"]
["","Manual përdorimi","","","","1","1","1","","1"]
["","Filtër ajri","","","","2","2","2","","2"]
["","Telekomandë me rreze infra të kuqe","","","","1","1","1","","1"]
["","Pllakë montimi telekomande","","","","1","1","1","","1"]
["","Qese vidash","","","","1","1","1","","1"]
["","Mbulesa e vidës","","","","1","1","1","","1"]
["","Bateri AAA me qeliza të thata","","","","2","2","2","","2"]
["","Masat e përgjithshme të sigurisë","","","","1","1","1","","1"]
["Agjenti ftohës","GWP","","","","675.0","675.0","675.0","","675.0"]
["Control systems","Wired remote control","","","","BRC073","BRC073","BRC073","","BRC073"]
["","Infrared remote control","","","","ARC466A58","ARC466A58","ARC466A58","","ARC466A58"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","6.35","6.35","6.35","","6.35"]
["","Gazi","","Dia. jasht.","mm","9.50","9.50","9.50","","12.70"]
["","Kullimi","","","","18","18","18","","18"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","0.020","0.022","0.023","","0.030"]
["","Ngrohje","","Nom.","kW","0.020","0.020","0.022","","0.039"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","57","57","60","","60"]
["Dimensionet","Njësia","","Gjerësia","mm","798","798","798","","798"]
["","","","Thellësia","mm","189","189","189","","189"]
["","","","Lartësia","mm","295","295","295","","295"]
["Casing","Ngjyra","","","","E bardhë","E bardhë","E bardhë","","E bardhë"]
["Pesha","Njësia","","","kg","11.50","11.50","11.50","","11.50"]
["Fan","Vëllimi i qarkullimit të ajrit","Ngrohje","I lartë","m³/min","10.9","11.1","11.5","","15.1"]
["","","","Medium","m³/min","8.7","9.0","9.0","","11.1"]
["","","","I ulët","m³/min","6.4","6.4","6.4","","8.2"]
["","","","Funksionim pa zhurmë","m³/min","4.5","4.5","4.5","","5.7"]
["","","Ftohje","I ulët","m³/min","6.1","6.1","6.1","","7.6"]
["","","","Medium","m³/min","8.2","8.6","8.6","","10.4"]
["","","","I lartë","m³/min","11.0","11.5","11.9","","13.5"]
["","","","Funksionim pa zhurmë","m³/min","4.6","4.6","4.6","","5.2"]
["Power supply","Faza","","","","1~","1~","1~","","1~"]
["","Emri","","","","V1","V1","V1","","V1"]
["","Frekuenca","","","Hz","50","50","50","","50"]
["","Tensioni","","","V","220-240","220-240","220-240","","220-240"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","","","","0.028"]
["","Ngrohje","","Nom.","kW","","","","0.036"]
["Veshja e jashtme","Ngjyra","","","","","","","E bardhë"]
["Dimensionet","Njësia","","Lartësia","mm","","","","295"]
["","","","Gjerësia","mm","","","","798"]
["","","","Thellësia","mm","","","","189"]
["Pesha","Njësia","","","kg","","","","11.50"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","","","","13.1"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","","","","9.8"]
["","","","I ulët","m³/min","","","","7.2"]
["","","","Funksionim pa zhurmë","m³/min","","","","4.6"]
["","","Ngrohje","I lartë","m³/min","","","","14.6"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","","","","10.5"]
["","","Ngrohje","I ulët","m³/min","","","","7.7"]
["","","","Funksionim pa zhurmë","m³/min","","","","5.2"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","","","","60"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","","","","45"]
["","","","Mesatar","dBA","","","","37"]
["","","","I ulët","dBA","","","","29"]
["","","","Funksionim pa zhurmë","dBA","","","","21"]
["","Ngrohje","","I lartë","dBA","","","","45"]
["","","","Mesatar","dBA","","","","37"]
["","","","I ulët","dBA","","","","29"]
["","","","Funksionim pa zhurmë","dBA","","","","21"]
["Agjenti ftohës","GWP","","","","","","","675.0"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","","","","6.35"]
["","Gazi","","Dia. jasht.","mm","","","","12.70"]
["","Kullimi","","","","","","","18"]
["Sistemet e kontrollit","Telekomandë me rreze infra të kuqe","","","","","","","ARC466A58"]
["","Telekomandë me tela","","","","","","","BRC073"]
["Aksesore Standarde","Installation manual","","","","","","","1"]
["","Screw cover","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","General safety precautions","","","","","","","1"]
["","Operation manual","","","","","","","1"]
["","Air filter","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Remote controller mounting plate","","","","","","","1"]
["","Screw bag","","","","","","","1"]
["Furnizimi me energji","Emri","","","","","","","V1"]
["","Faza","","","","","","","1~"]
["","Frekuenca","","","Hz","","","","50"]
["","Tensioni","","","V","","","","220-240"]