{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXC-A"]
[]
[]
[]
[]
["","","","","FTXC25AV1B","FTXC35AV1B","FTXC50AV1B","FTXC60AV1B"]
["Niveli i presionit të zhurmës","Ftohje","Funksionim pa zhurmë","dBA","21","22","32","33"]
["","","Super i lartë","dBA","41","42","44","46"]
["","","I ulët","dBA","29","30","35","37"]
["","","I lartë","dBA","40","41","40","43"]
["Aksesore Standarde","Manual instalimi","","","Manual instalimi","Manual instalimi","Manual instalimi","Manual instalimi"]
["","Manual përdorimi","","","Manual përdorimi","Manual përdorimi","Manual përdorimi","Manual përdorimi"]
["","Telekomandë me valë","","","Telekomandë me valë","Telekomandë me valë","Telekomandë me valë","Telekomandë me valë"]
["","Bateri","","","Bateri","Bateri","Bateri","Bateri"]
["","Mbajtës telekomande","","","Mbajtës telekomande","Mbajtës telekomande","Mbajtës telekomande","Mbajtës telekomande"]
["","Pllakë montimi","","","Pllakë montimi","Pllakë montimi","Pllakë montimi","Pllakë montimi"]
["","Filtra me apatit titani","","","Filtra me apatit titani","Filtra me apatit titani","Filtra me apatit titani","Filtra me apatit titani"]
["Lidhjet e tubacioneve","Lëngu","Dia. jasht.","mm","6.35","6.35","6.35","6.35"]
["","Gazi","Dia. jasht.","mm","9.5","9.5","12.7","12.7"]
["","Kullimi","","","OD16,5","OD16,5","OD16,5","OD16,5"]
["Power input","Ftohje","Nom.","kW","693","1,060","1,668","1,931"]
["","Ngrohje","Nom.","kW","700","950","1,550","1,680"]
["Sound power level","Ftohje","","dBA","53","54","55","61"]
["Dimensionet","Njësia","Gjerësia","mm","859","859","1,124","1,124"]
["","","Thellësia","mm","209","209","237","237"]
["","","Lartësia","mm","288","288","310","310"]
["Veshja e jashtme","Materiali","","","Polistiren për goditje të forta","Polistiren për goditje të forta","Polistiren për goditje të forta","Polistiren për goditje të forta"]
["","Ngjyra","","","E bardhë","E bardhë","E bardhë","E bardhë"]
["Pesha","Njësia","","kg","9.0","9.0","14.0","14.0"]
["Ventilatori","Presioni i jashtëm statik","I lartë","Pa","0","0","0","0"]
["","","Nom.","Pa","0","0","0","0"]
["","","I ulët","Pa","0","0","0","0"]
["","","Super i lartë","Pa","0","0","0","0"]
["Power supply","Faza","","","1~","1~","1~","1~"]
["","Frekuenca","","Hz","50","50","50","50"]
["","Emri","","","V1","V1","V1","V1"]
["","Tensioni","","V","220-240","220-240","220-240","220-240"]